- Top
- Preparation
- Connecting a microphone
- When mounting a microphone holder (optional) for use

When mounting a microphone holder (optional) for use

1. Remove the screws on the microphone holder mounting position and mount the microphone holder AJ-MH800G (optional). (Fig. 1)
2. Mount the microphone and tighten the clamping screw. (Fig. 2)
3. Loosen the lock lever, adjust the angle of the microphone, and then tighten the lock lever. (Fig. 3)
4. Insert the microphone cable into the cable clamp and connect it to the <MIC> terminal (front). (Fig. 4)
5. Set the <LINE/MIC/+48V> selector switch (<FRONT MIC>) to <MIC> or <+48V>.

Top of the page