- Top
- Menu Operations
- Menu list
- [RETURN SETTING]

[RETURN SETTING]

Item | Description of settings
[RETURN MODE] | Sets the operation mode of the <RET> switch. [NORM], [TOGGLE], [BOX] Factory setting: [NORM]
[RETURN SELECT] | [RETURN A] | Sets the function assigned to return A. [RETURN1], [RETURN2] Factory setting: [RETURN1]
[RETURN B] | Sets the function assigned to return B. [RETURN1], [RETURN2] Factory setting: [RETURN2]
[RETURN C] | Sets the function assigned to return C. [RETURN1], [RETURN2] Factory setting: [RETURN1]
[RETURN1 ID] | Sets the name of return video 1. (5 characters or less) Factory setting: [RET1.]
[RETURN2 ID] | Sets the name of return video 2. (5 characters or less) Factory setting: [RET2.]

Top of the page