- Top
- Description of Parts
- Rear side

Rear side

1. <CALL> lamp
2. Lights up in green when the call switch is pressed from the ROP or CCU.
3. <CALL> switch
4. While this switch is pressed, the call lamps on the ROP and CCU are lit and the ROP buzzer sounds. (When the ROP buzzer setting is enabled)

   NOTE If the <CALL> switch is pressed when the camera is operating with an external DC power source, the ROP call lamp does not light up.

5. <TALK> switch (<INTERCOM>)
6. This switch is the <ON>/<OFF>/<PTT> selector switch of the intercom microphone connected to the <INTERCOM> terminal.
7. Pushes the switch towards <ON>/<PTT> to turn on the microphone.
8. <INTERCOM> terminal
9. Used to connect the intercom or headset plug.
10. <LINE/MIC/+48V> selector switch (<FRONT MIC>)
11. Used to switch the audio input signal of the audio channel 1.
12. <LINE>: When connecting audio equipment with the line input
13. <MIC>: When connecting an external microphone
14. <+48V>: When supplying 48 V power to the microphone
15. <LINE/MIC/+48V> selector switch (<MIC 2>)
16. Used to switch the audio input signal of the audio channel 2.
17. <LINE>: When connecting audio equipment with the line input
18. <MIC>: When connecting an external microphone
19. <+48V>: When supplying 48 V power to the microphone
20. Back tally lamp
21. Lights up when the tally signal is supplied.
22. R tally signal: Lit in red
23. G tally signal: Lit in green
24. R and G tally signals at the same time: Lit in red
25. Back tally lamp selector switch
26. Used to switch the back tally lamp to on/off.
27. Rear viewfinder terminal
28. Used to connect the 9-inch LCD viewfinder AK-HVF100G.
29. This D-sub connector is used for the viewfinder interface.

    NOTE AK-HVF70G, AK-HVF75G can also be connected to this terminal.

30. <OPT> lamp
31. Indicates the camera’s optical signal reception status.
32. Normal: Lit in green
33. Error: Lit in red

    NOTE When an error has occurred, turn off the power of this camera and the CCU, and then clean the optical fiber connector. If the error persists, immediately turn off the power, and contact your dealer.

34. <PGM> dial (<INTERCOM>)
35. Adjusts the mix level of the intercom and PGM.
36. <LEVEL> dial (<INTERCOM>)
37. Used to adjust the volume level of the intercom when the mixing function of the intercom connected to the <INTERCOM> terminal and the PGM is enabled. The mixing function of the intercom and the PGM can be enabled/disabled from [MAIN MENU] → [INTERCOM SETTING] → [INCOM RECEIVE SETTING] → [PGM MIX]
38. <HD SDI1> terminal (BNC)
39. [CAM]: Outputs camera images.
40. [HD PROMPT]: Outputs HD prompter video images.
41. Configure the output images in [MAIN MENU] → [IN/OUT SELECT] → [HD‑SDI1 OUT].

    NOTE Use a cable that is 5C-FB or above. [HD PROMPT] can be selected only when the camera is connected to the CCU. Please also note that the video formats available for output are 1080/59.94p/50p/59.94i/50i.

42. <HD SDI2> terminal (BNC)
43. [CAM]: Outputs camera images.
44. [VF]: Outputs viewfinder images.
45. [RET]: Outputs return images.
46. [RET1]/[RET2]: Outputs the selected images.
47. Configure the output images in [MAIN MENU] → [IN/OUT SELECT] → [HD‑SDI2 OUT].

    NOTE Use a cable that is 5C-FB or above. [RET] and [RET1]/[RET2] can be selected only when the camera is connected to the CCU.

48. <AUX> terminal
49. This is the external device connecting terminal.
50. [PMT OUT]: Outputs prompter video images.
51. [HD TRUNK]: HD trunk input
52. Set this from [MAIN MENU] → [IN/OUT SELECT] → [AUX I/O].

    NOTE Use a cable that is 5C-FB or above. The video formats available for input to [HD TRUNK] are 1080/59.94p/50p/59.94i/50i.

53. <DC IN> terminal
54. This is an input terminal for the external DC power supply. Connect an external DC power supply to this terminal. (DC 10.8 V to 17 V)
55. <MIC 2> terminal
56. Used to connect audio equipment or a microphone.
57. The power for the microphone is supplied via this terminal, enabling use of a phantom powered (48 V) microphone. Turn the power off when connecting a microphone, and then configure the settings to suit the microphone after connecting the microphone.

Top of the page