- Top
- Overview
- Using the camera in a system
- Basic configuration devices

Basic configuration devices

The basic system configuration includes the lens, HD Studio Camera, viewfinder, Camera Control Unit (CCU), and Remote Operation Panel (ROP).

Part name | Part No. | Remark
1.5-inch HD viewfinder | AJ-CVF50G | This is the viewfinder for HD Studio Camera.
3.45-inch color viewfinder | AG-CVF10G AG-CVF15G AJ-CVF25G | —
7-inch LCD color viewfinder | AK-HVF75G | —
9-inch LCD color viewfinder | AK-HVF100G | This is the LCD viewfinder for HD Studio Camera.
Lens | FUJINON/CANON | —
Camera Control Unit (CCU) | AK-HCU250P/AK-HCU250PS/AK-HCU250E/AK-HCU250ES | This is the camera control unit for HD Studio Camera. It is connected to HD Studio Camera using an optical fiber multi cable. Do not connect anything other than AK-HCU250P/AK-HCU250PS/AK-HCU250E/AK-HCU250ES.
Remote Operation Panel (ROP) | AK-HRP1000G AK-HRP1005G AK-HRP1010G AK-HRP1015G AK-HRP250G | This is connected to the CCU using the ROP cable to remotely control the camera, CCU, and lens.

Top of the page