- Top
- Menu Operations
- Menu list
- [INTERCOM SETTING]

# [INTERCOM SETTING]

## [INTERCOM1]

Item | Description of settings
--- | ---
[INCOM1 TALK SETTING] | [MIC TYPE] | Selects the type of the intercom 1 microphone. [DYN]: Dynamic type [ECM]: Condenser type [CBN]: Carbon type Factory setting: [DYN]
| [MIC POWER] | Sets the on/off for the power supply to the intercom 1 microphone. [OFF], [ON] Factory setting: [OFF]
| [MIC GAIN] | Sets the volume of the intercom 1 microphone. [−12dB]…[12dB] Factory setting: [0dB]
| [SIDE TONE] | Sets the volume of the intercom 1 microphone side tone. [OFF], [−36dB]…[0dB] (3 dB step) Factory setting: [−6dB]
| [INCOM1 TO CCU] | Sets whether to transmit the intercom 1 microphone audio to the CCU. [OFF], [ON] Factory setting: [ON]
[INCOM1 RECEIVE SETTING] | [OUTPUT GAIN] | Sets the gain of the intercom 1 audio output. [NORMAL], [BOOST] Factory setting: [NORMAL]
| [OUTPUT CH] | Sets the allocation of the intercom 1 audio output. [CH1/CH2], [CH2/CH1] Factory setting: [CH1/CH2]
[INCOM1 RECEIVE CH1 SETTING] | [PGM1 MIX] | Sets whether to mix the PGM1 signal with the intercom 1 CH1 output. [OFF], [ON] Factory setting: [ON]
| [PGM2 MIX] | Sets whether to mix the PGM2 signal with the intercom 1 CH1 output. [OFF], [ON] Factory setting: [ON]
| [CRANE INCOM MIX] | Sets whether to mix the crane intercom signal with the intercom 1 CH1 output. [OFF], [ON] Factory setting: [OFF]
| [INCOM2 MIX] ([CLEAR COM MIX]) | Sets whether to mix the intercom 2 signal (CLEAR COM signal for the Clear-Com option) with the intercom 1 CH1 output. [OFF], [ON] Factory setting: [OFF]
[INCOM1 RECEIVE CH2 SETTING] | [ENG MIX] | Sets whether to mix the ENG signal with the intercom 1 CH2 output. [OFF], [ON] Factory setting: [OFF]
| [PROD MIX] | Sets whether to mix the PROD signal with the intercom 1 CH2 output. [OFF], [ON] Factory setting: [OFF]
| [PGM1 MIX] | Sets whether to mix the PGM1 signal with the intercom 1 CH2 output. [OFF], [ON] Factory setting: [ON]
| [PGM2 MIX] | Sets whether to mix the PGM2 signal with the intercom 1 CH2 output. [OFF], [ON] Factory setting: [ON]
| [CRANE INCOM MIX] | Sets whether to mix the crane intercom signal with the intercom 1 CH2 output. [OFF], [ON] Factory setting: [OFF]
| [INCOM2 MIX] ([CLEAR COM MIX]) | Sets whether to mix the intercom 2 signal (CLEAR COM signal for the Clear-Com option) with the intercom 1 CH2 output. [OFF], [ON] Factory setting: [OFF]

## [INTERCOM2]

This item is not displayed when Clear-Com is connected.

Item | Description of settings
--- | ---
[INCOM2 TALK SETTING] | [MIC TYPE] | Selects the type of the intercom 2 microphone. [DYN]: Dynamic type [ECM]: Condenser type [CBN]: Carbon type Factory setting: [DYN]
| [MIC POWER] | Sets the on/off for the power supply to the intercom 2 microphone. [OFF], [ON] Factory setting: [OFF]
| [MIC GAIN] | Sets the volume of the intercom 2 microphone. [−12dB]…[+12dB] Factory setting: [0dB]
| [SIDE TONE] | Sets the volume of the intercom 2 microphone side tone. [OFF], [−36dB]…[0dB] Factory setting: [−6dB]
| [INCOM2 TO CCU] | Sets whether to transmit the intercom 2 microphone audio to the CCU. [OFF], [ON] Factory setting: [ON]
[INCOM2 RECEIVE SETTING] | [OUTPUT GAIN] | Sets the gain of the intercom 2 audio output. [NORMAL], [BOOST] Factory setting: [NORMAL]
| [OUTPUT CH] | Sets the allocation of the intercom 2 audio output. [CH1/CH2], [CH2/CH1] Factory setting: [CH1/CH2]
[INCOM2 RECEIVE CH1 SETTING] | [PGM1 MIX] | Sets whether to mix the PGM1 signal with the intercom 2 CH1 output. [OFF], [ON] Factory setting: [ON]
| [PGM2 MIX] | Sets whether to mix the PGM2 signal with the intercom 2 CH1 output. [OFF], [ON] Factory setting: [ON]
| [CRANE INCOM MIX] | Sets whether to mix the crane intercom signal with the intercom 2 CH1 output. [OFF], [ON] Factory setting: [OFF]
| [INCOM1 MIX] | Sets whether to mix the intercom 1 signal with the intercom 2 CH1 output. [OFF], [ON] Factory setting: [OFF]
[INCOM2 RECEIVE CH2 SETTING] | [ENG MIX] | Sets whether to mix the ENG signal with the intercom 2 CH2 output. [OFF], [ON] Factory setting: [OFF]
| [PROD MIX] | Sets whether to mix the PROD signal with the intercom 2 CH2 output. [OFF], [ON] Factory setting: [OFF]
| [PGM1 MIX] | Sets whether to mix the PGM1 signal with the intercom 2 CH2 output. [OFF], [ON] Factory setting: [ON]
| [PGM2 MIX] | Sets whether to mix the PGM2 signal with the intercom 2 CH2 output. [OFF], [ON] Factory setting: [ON]
| [CRANE INCOM MIX] | Sets whether to mix the crane intercom signal with the intercom 2 CH2 output. [OFF], [ON] Factory setting: [OFF]
| [INCOM1 MIX] | Sets whether to mix the intercom 1 signal with the intercom 2 CH2 output. [OFF], [ON] Factory setting: [OFF]

## [STANDBY INTERCOM]

Item | Description of settings
--- | ---
[STBY INCOM SETTING] | [INPUT LEVEL] | Sets the input signal level of the stand-by intercom. [−36dB]…[+12dB] Factory setting: [0dB]
| [OUTPUT LEVEL] | Sets the output signal level of the stand-by intercom. [−36dB]…[+12dB] Factory setting: [0dB]
| [CANCEL LEVEL] | Sets the input/output cancel signal level of the stand-by intercom. [−20.0dB]…[+20.0dB] (0.5 dB step) Factory setting: [0.0dB]
| [STBY INCOM ON/OFF] | Enables/disables the stand-by intercom. [OFF], [ON] Factory setting: [ON]

## [CRANE INTERCOM]

Item | Description of settings
--- | ---
[CRANE INCOM SETTING] | [INPUT LEVEL] | Sets the input volume of the crane intercom (connected to the <EXT I/O> terminal). [−36dB]…[+12dB] Factory setting: [0dB]
| [OUTPUT LEVEL] | Sets the output volume of the crane intercom (connected to the <EXT I/O> terminal). [−36dB]…[+12dB] Factory setting: [0dB]
| [SIDE TONE] | Sets the side tone volume of the crane intercom (connected to the <EXT I/O> terminal). [OFF], [−36dB]…[0dB] (3 dB step) Factory setting: [−6dB]
| [ENG/PROD] | Sets the line input of the crane intercom audio. [ENG], [PROD], [BOTH] Factory setting: [ENG]
| [CRANE TO CCU] | Sets whether to output the crane intercom audio to the CCU. [OFF], [ON] Factory setting: [OFF]
[CRANE INCOM OUTPUT SETTING] | [PGM1 MIX] | Sets whether to mix the PGM1 signal with the crane intercom output. [OFF], [ON] Factory setting: [ON]
| [PGM2 MIX] | Sets whether to mix the PGM2 signal with the crane intercom output. [OFF], [ON] Factory setting: [ON]
| [INCOM1 MIX] | Sets whether to mix the intercom 1 signal with the crane intercom output. [OFF], [ON] Factory setting: [OFF]
| [INCOM2 MIX] ([CLEAR COM MIX]) | Sets whether to mix the intercom 2 signal (CLEAR COM signal for Clear-Com option) with the crane intercom output. [OFF], [ON] Factory setting: [OFF]

## [CLEAR COM]

This item is not displayed when intercom 2 is connected.

Item | Description of settings
--- | ---
[CLEAR COM SETTING] | [INPUT LEVEL] | Sets the input volume of Clear-Com. [−36dB]…[+12dB] Factory setting: [0dB]
| [CANCEL LEVEL] | Sets the input/output cancel signal level of Clear-Com. [−20.0dB]…[+20.0dB] (0.5 dB step) Factory setting: [0.0dB]
| [SIDE TONE] | Sets the side tone volume of Clear-Com. [OFF], [−36dB]…[0dB] (3 dB step) Factory setting: [−6dB]
| [CLEAR COM TO CCU] | Sets whether to output the Clear-Com audio to the CCU. [OFF], [ON] Factory setting: [ON]
[CLEAR COM OUTPUT SETTING] | [PGM1 MIX] | Sets whether to mix the PGM1 signal with Clear-Com output. [OFF], [ON] Factory setting: [ON]
| [PGM2 MIX] | Sets whether to mix the PGM2 signal with Clear-Com output. [OFF], [ON] Factory setting: [ON]
| [INCOM1 MIX] | Sets whether to mix the INCOM1 signal with Clear-Com output. [OFF], [ON] Factory setting: [OFF]
| [CRANE INCOM MIX] | Sets whether to mix the CRANE INCOM signal with Clear-Com output. [OFF], [ON] Factory setting: [OFF]

## [EAR PHONES SETTING]

Item | Description of settings
--- | ---
[LCH OUTPUT SELECT] | Sets the audio signal output to the L channel of the earphones. [INCOM1(CH1)], [INCOM2(CH1)] (for Clear-Com option: [CLEAR COM]), [INCOM1/2 MIX(CH1)] (for Clear-Com option: [INCOM1(CH1)/CLEAR COM MIX]), [PGM1], [PGM2], [PGM1/PGM2 MIX], [MIC1], [OFF] Factory setting: [INCOM1(CH1)]
[RCH OUTPUT SELECT] | Sets the audio signal output to the R channel of the earphones. [INCOM1(CH2)], [INCOM2(CH2)] (for Clear-Com option: [CLEAR COM]), [INCOM1/2 MIX(CH2)] (for Clear-Com option: [INCOM1(CH2)/CLEAR COM MIX]), [PGM1], [PGM2], [PGM1/PGM2 MIX], [MIC2], [OFF] Factory setting: [INCOM1(CH2)]
[LCH MONITOR LEVEL] | Sets the monitor output level for the L channel of the earphones. [−40dB]…[+12dB] Factory setting: [0dB]
[RCH MONITOR LEVEL] | Sets the monitor output level for the R channel of the earphones. [−40dB]…[+12dB] Factory setting: [0dB]

## [PGM OUTPUT]

These items can be set only when the PGM option is used.

Item | Description of settings
--- | ---
[PGM OUTPUT SELECT] | Sets the audio output from the <PGM OUT> terminal. [PGM1], [PGM2], [PGM1/PGM2], [ENG], [PROD], [ENG/PROD], [CRANE] Factory setting: [PGM1]
[PGM OUTPUT LEVEL] | Sets the output level from the <PGM OUT> terminal. [−36dB]…[+12dB] Factory setting: [0dB]

## [LEVEL/PGM1/PGM2 VR SETTING]

Item | Description of settings
--- | ---
[INTERCOM1 PGM1 VR] | Sets the audio signal to be controlled by the <PGM1> dial of <INTERCOM1>. [ENG], [PROD], [ENG/PROD], [PGM1], [PGM2], [PGM1/PGM2], [CRANE], [INCOM2] (for Clear-Com option: [CLEAR COM]) Factory setting: [PGM1]
[INTERCOM1 PGM2 VR] | Sets the audio signal to be controlled by the <PGM2> dial of <INTERCOM1>. [ENG], [PROD], [ENG/PROD], [PGM1], [PGM2], [PGM1/PGM2], [CRANE], [INCOM2] (for Clear-Com option: [CLEAR COM]) Factory setting: [PGM2]
[INTERCOM2 PGM1 VR] | Sets the audio signal to be controlled by the <PGM1> dial of <INTERCOM2>. [ENG], [PROD], [ENG/PROD], [PGM1], [PGM2], [PGM1/PGM2], [CRANE], [INCOM1] Factory setting: [PGM1]
[INTERCOM2 PGM2 VR] | Sets the audio signal to be controlled by the <PGM2> dial of <INTERCOM2>. [ENG], [PROD], [ENG/PROD], [PGM1], [PGM2], [PGM1/PGM2], [CRANE], [INCOM1] Factory setting: [PGM2]
[VR MIN MODE] | Sets the level when the volume level is minimum. [MUTE]: Muted [MIN GAIN]: Minimum level Factory setting: [MUTE]
[B/U INTERCOM LEVEL] | Sets the audio signal to be controlled by the intercom level of the Build-up Unit. [OFF], [INCOM1], [INCOM2] (for Clear-Com option: [CLEAR COM]), [INCOM1/INCOM2] (for Clear-Com option: [INCOM1/CLEAR COM]) Factory setting: [OFF]

## [OPT INTERCOM INPUT SETTING]

Item | Description of settings
--- | ---
[OPT ENG INPUT LEVEL] | Sets the input level of the ENG audio signal sent from the CCU to the camera. [−36dB]…[+12dB] Factory setting: [0dB]
[OPT PROD INPUT LEVEL] | Sets the input level of the PROD audio signal sent from the CCU to the camera. [−36dB]…[+12dB] Factory setting: [0dB]
[OPT PGM1 INPUT LEVEL] | Sets the input level of the PGM1 audio signal sent from the CCU to the camera. [−36dB]…[+12dB] Factory setting: [0dB]
[OPT PGM2 INPUT LEVEL] | Sets the input level of the PGM2 audio signal sent from the CCU to the camera. [−36dB]…[+12dB] Factory setting: [0dB]

Top of the page