- Top
- Description of Parts
- Right side

# Right side

1. <USB2.0> terminal (host)

   Used to connect the USB 2.0 cable.

   NOTE

   - Use a double-shielded cable when connecting a cable to the <USB2.0> terminal.

2. <OPT FIBER> terminal

   Used to connect with the CCU using the optical fiber multi cable. When the terminal is not in use, attach the dust cap.

3. <LAN> terminal

   Used to connect the LAN cable (100BASE-TX/1000BASE-T).

   NOTE

   - Use a shielded cable when connecting a cable to the <LAN> terminal.

4. Shoulder pad

   Reduces the burden on the shoulder when the camera is carried on your shoulder.

5. Slide lock release lever

   Releases this lever when changing the shoulder pad position.

6. Shoulder strap fittings

   Used to attach the shoulder strap.

7. <VF> terminal

   Used to connect the plug of the viewfinder.

8. Camera number sheet holder

   Attach the supplied camera number sheet.

9. <USER 3> button

   A user-selected function can be assigned to this button. Pressing the button performs the assigned function.

10. <LENS> terminal

    Used to connect the lens cable.

Top of the page