- Top
- Preparation
- Data

# Data

The following shows the data handled in the camera.

Managed system component | Name | Quantity | Description
--- | --- | --- | ---
Camera | User file | 1 - 3 | These files contain equipment configuration data held by the camera, set in [MAIN MENU]. The data is managed by the camera. It can be saved or loaded by [MAIN MENU] → [FILE] → [USER FILE].
Lens file | 1 - 32 | These files contain data used by video engineers to correct characteristics specific to each lens. The data is managed by the camera. It can be saved or loaded by [MAIN MENU] → [MAINTENANCE] → [LENS FILE ADJUST].
CAC file | 1 - 32 | These files contain chromatic aberration compensation data specific to the lens. The data is managed by the camera. It can be loaded from a memory card by [MAIN MENU] → [FILE] → [CAC FILE].
Scene file | 1 - 8 | These files which contain data for creating pictures are handled mainly by video engineers. The data is managed by the camera. It can be loaded by [MAIN MENU] → [FILE] → [SCENE FILE].
Operation file | 1 | These files which contain operation data are handled mainly by camera operators. The data is managed by the camera. It can be saved or loaded by [MAIN MENU] → [FILE] → [SD CARD] using a memory card.
Reference file | 1 - 3 | These files contain data excluding the operation data from the equipment configuration data. The data is managed by the camera. It can be saved or loaded by [MAIN MENU] → [FILE] → [REFERENCE FILE].

User file
CAC file
Top of the page