- Top
- Preparation
- On-screen displays of the viewfinder

# On-screen displays of the viewfinder

Studio Handy Camera settings and messages indicating operating statuses appear on the viewfinder screen.

All items that can be displayed are located as follows.

1. Camera mode display

   Indicates the camera image mode.

   - [59.94p]

   - [50p]

   - [29.97p]

   - [23.98p]

   - [25p]

2. HDR mode display

   Displayed when the format is HDR.

3. System mode display

   Indicates the system frequency.

   - [1080/59.94p]

   - [1080/50p]

   - [1080/29.97p]

   - [1080/25p]

   - [1080/23.98p]

   - [1080/59.94p-240fps]

   - [1080/50p-200fps]

4. Warning display (preheating)

   Displayed when the device is being preheated at startup due to low temperature inside the device.

5. Warning display (device)

   Displayed when there is an abnormality with the condition of the device.

   - The fan stops abnormally.

   - Internal temperature becomes high.

   - DC output supply goes over. (Combined total of each output)

   - There is a problem with the light reception level.

   The display cannot be hidden.

6. Warning display (fan stopped)

   Displayed when the fan is stopped.

   [MAIN MENU] → [MAINTENANCE] → [FAN SETTING] → [FAN] → [FAN MODE] → [OFF] is set.

7. Warning display (menu display)

   Displays the camera menu in the CCU. The menu cannot be operated from the camera.

8. Return ID display

   Displays the return ID of the current return output number.

   The ID (character string) set in [MAIN MENU] → [RETURN SETTING] → [RETURN1 ID] to [RETURN4 ID] is displayed.

   The following return IDs (character strings) are set in factory settings.

   - [RET1] (When [RETURN1] is output)

   - [RET2] (When [RETURN2] is output)

   - [RET3] (When [RETURN3] is output)

   - [RET4] (When [RETURN4] is output)

9. Monitor output signal display

   Indicates the signal type that is output to the monitor screen.

   Configures the signal settings from [MAIN MENU] → [IN/OUT SELECT] → [VF OUT].

   - [R]

   - [G]

   - [B]

   - [Y/C]

   - [NAM]

10. High-sensitivity mode display

    Displayed when [MAIN MENU] → [SYSTEM MODE] → [SHOOTING MODE] → [HIGH SENS] is set.

11. Voltage display

    Indicates the voltage coming in from the power supply.

12. Focus assist magnification display

    The focus assist magnification display function is displayed while active.

13. ND filter display

    Indicates the selected ND filter value.

    - [1]

    - [2]

    - [3]

    - [4]

    - [5]

14. CC filter display

    Indicates the selected CC filter value.

    - [A]

    - [B]

    - [C]

    - [D]

    - [E]

15. <WHITE BAL> switch position display

    Indicates the selected switch position.

    - [A]: When the <WHITE BAL> switch is set to <A>

    - [B]: When the <WHITE BAL> switch is set to <B>

    - [P]: When the <WHITE BAL> switch is set to <PRST>

16. Color temperature display

    Indicates the color temperature that is set on the camera.

    This can be either the memory value when automatic white balance is performed or the value configured in the menu.

17. Shutter speed display

    Indicates the shutter speed in accordance with each setting.

    When [MAIN MENU] → [SWITCH MODE] → [SHUTTER SPEED] → [SHUTTER SW] → [ON] is set, and also [MAIN MENU] → [SWITCH MODE] → [SHUTTER SPEED] → [SHUTTER MODE] → [SHUTTER] is set

    - [1/48] (in [23.98p] mode only)

    - [1/50] (in [25p] mode only)

    - [1/60] (in [50i]/[50p]/[29.97p]/[25p]/[23.98p] mode only)

    - [1/100]

    - [1/120] (in [59.94i]/[59.94p]/[29.97p]/[23.98p] mode only)

    - [1/125]

    - [1/250]

    - [1/500]

    - [1/1000]

    - [1/1500]

    - [1/2000]

    When [MAIN MENU] → [SWITCH MODE] → [SHUTTER SPEED] → [SHUTTER SW] → [ON] is set, and also [MAIN MENU] → [SWITCH MODE] → [SHUTTER SPEED] → [SHUTTER MODE] → [SYNCHRO] is set

    - [61.7Hz] to [6130Hz] (in [59.94i]/[59.94p] mode only)

    - [51.5Hz] to [6250Hz] (in [50i]/[50p] mode only)

    - [30.9Hz] to [2600Hz] (in [29.97p] mode only)

    - [25.7Hz] to [3130Hz] (in [25p] mode only)

    - [24.7Hz] to [2880Hz] (in [23.98p] mode only)

    - [240Hz] to [6130Hz] (in [240fps] mode only)

    - [200Hz] to [6250Hz] (in [200fps] mode only)

    When [MAIN MENU] → [SWITCH MODE] → [SHUTTER SPEED] → [SHUTTER SW] → [OFF] is set

    - [SH.OFF]

18. Master gain display

    Indicates the value set in [MAIN MENU] → [SWITCH MODE] → [GAIN SETTING] → [LOW GAIN]/[MID GAIN]/[HIGH GAIN].

    - [−6dB] to [36dB]

19. Offset gain display

    Indicates the value set in [MAIN MENU] → [SWITCH MODE] → [GAIN SETTING] → [OFFSET LOW GAIN]/[OFFSET MID GAIN]/[OFFSET HIGH GAIN].

    - [−2.9dB] to [+2.9dB]

20. Flash band compensation display

    Displayed when the flash band compensation function is active.

21. Dynamic range stretcher display

    Displayed when the dynamic range stretcher function is active.

22. Chromatic aberration compensation display

    Displayed when the chromatic aberration compensation function is active.

23. Digital extender display

    Displayed when the digital extender is being used.

24. Lens extender display

    Displayed when the lens extender is being used.

25. Iris display

    Indicates the iris setting value (F value) or [OPEN]/[CLOSE]. The F value is an approximate value.

    [NC] is displayed when the lens cable is not connected.

26. F drop display

    Displayed when the F drop has occurred.

    NOTE

    - The display may not be supported depending on the lens model.

      For details, consult the lens manufacturer.

27. Zoom position display

    Indicates the zoom position.

    - [Z00] to [Z99]

    NOTE

    - The zoom position is displayed when using a lens having a zoom position output.

28. Focus position display

    Indicates the focus position.

    - [00] to [99]

    NOTE

    - The focus position is displayed when using a lens having a focus position output.

29. Focus information display

    Displays the focus information of the focus.

    NOTE

    - This is displayed only when an auto focus lens with the function to return the focus information is mounted.

30. Level gauge display

    Displays the tilt of the camera in horizontal direction or vertical direction.

31. Optical level display

    Indicates the level of the optical signals the camera will receive.

32. Camera warning and information display area

    Displays a message indicating the occurrence of an error, the camera settings, the progress made in the adjustments, or the adjustment results for about three seconds.

33. Audio input channel and level meter

    Indicates the audio level of the <MIC 1> terminal (audio input 1) and <MIC 2> terminal (audio input 2).

Top of the page