- Top
- Menu Operations
- Menu list
- [PAINT]

# [PAINT]

## [PAINT SWITCH]

Item | Description of settings
--- | ---
[BLACK SHADING] | Enables/disables the black shading (saw-toothed waveform or parabolic waveform). [OFF], [ON] Factory setting: [ON]
[WHITE SHADING] | Enables/disables the white shading (saw-toothed waveform or parabolic waveform). [OFF], [ON] Factory setting: [ON]
[FLARE] | Enables/disables flare. [OFF], [ON] Factory setting: [ON]
[GAMMA] | Enables/disables gamma. [OFF], [ON] Factory setting: [ON]
[BLACK GAMMA] | Enables/disables black gamma. [OFF], [ON] Factory setting: [OFF]
[KNEE] | Enables/disables knee. [OFF], [ON] Factory setting: [ON]
[WHITE CLIP] | Enables/disables white clips. [OFF], [ON] Factory setting: [ON]
[DRS SW] | Enables/disables dynamic range stretcher. [OFF], [ON] Factory setting: [OFF]
[DETAIL] | Enables/disables the detail. [OFF], [ON] Factory setting: [ON]
[SKIN TONE DETAIL] | Enables/disables the skin tone detail. [OFF], [ON] Factory setting: [OFF]
[MATRIX] | Enables/disables matrix (linear matrix/12-axis color correction). [OFF], [ON] Factory setting: [OFF]
[LINEAR MATRIX] | Enables/disables linear matrix. [OFF], [ON] Factory setting: [OFF]
[COLOR CORRECT] | Enables/disables 12-axis color correction. [OFF], [ON] Factory setting: [OFF]
[PRESET MATRIX] | Sets the preset matrix. [NORM], [EBU], [NTSC] Factory setting: [NORM]

## [BLACK SHADING]

Item | Description of settings
--- | ---
[CORRECT] | Enables/disables black shading (saw-toothed waveform or parabolic waveform) correction. [OFF], [ON] Factory setting: [ON]
[H SAW R] | Adjusts the black shading gain for Rch horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[H SAW G] | Adjusts the black shading gain for Gch horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[H SAW B] | Adjusts the black shading gain for Bch horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[H PARA R] | Adjusts the black shading gain for Rch horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[H PARA G] | Adjusts the black shading gain for Gch horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[H PARA B] | Adjusts the black shading gain for Bch horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[V SAW R] | Adjusts the black shading gain for Rch vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[V SAW G] | Adjusts the black shading gain for Gch vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[V SAW B] | Adjusts the black shading gain for Bch vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[V PARA R] | Adjusts the black shading gain for Rch vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[V PARA G] | Adjusts the black shading gain for Gch vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[V PARA B] | Adjusts the black shading gain for Bch vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]

## [PEDESTAL]

Item | Description of settings
--- | ---
[MASTER PEDESTAL] | Adjusts the black level of the master pedestal. For relative value display: [−99]…[99] For absolute value display: [−5.6%]…[58.4%] Factory setting: [0]/[0%]
[R PEDESTAL] | Sets the correction level of red to the master pedestal. [−800]…[+800] Factory setting: [0]
[G PEDESTAL] | Sets the correction level of green to the master pedestal. [−800]…[+800] Factory setting: [0]
[B PEDESTAL] | Sets the correction level of blue to the master pedestal. [−800]…[+800] Factory setting: [0]
[PEDESTAL OFFSET] | Sets whether to maintain the Rch, Gch, and Bch pedestal levels after adjusting the automatic black balance. [ON]: Maintains the values set in [R PEDESTAL], [G PEDESTAL], and [B PEDESTAL]. [OFF]: Sets [R PEDESTAL], [G PEDESTAL], and [B PEDESTAL] to [0]. Factory setting: [OFF]
[MASTER PEDESTAL ABS DISP SWITCH] | Sets the display of [MASTER PEDESTAL]. This cannot be set in HDR mode. [ON]: Absolute value [OFF]: Relative value Factory setting: [OFF]
[MASTER PEDESTAL RANGE] | Sets the variable amount of the master pedestal. [NORMAL]: Current variable amount [WIDE]: Double of current variable amount Factory setting: [NORMAL]

## [CHROMA]

Item | Description of settings
--- | ---
[CHROMA LEVEL SWITCH] | Enables/disables the gain adjustment of chroma. [OFF], [ON] Factory setting: [OFF]
[CHROMA LEVEL] | Sets the gain adjustment of chroma. [−100%]…[+40%] Factory setting: [0%]

## [COLOR TEMP SETTING]

Item | Description of settings
--- | ---
[COLOR TEMP PRESET] | [COLOR TEMP PRE SWITCH] | Enables/disables the color temperature adjustment. [OFF], [ON] Factory setting: [OFF]
| [COLOR TEMP] | Sets the color temperature when [COLOR TEMP PRE SWITCH] is [ON]. When the <CC> filter is set to <B><3200K>: [2000K]…[15000K] When the <CC> filter is set to <C><4300K>: [2300K]…[99999K] When the <CC> filter is set to <D><6300K>: [2700K]…[99999K] Factory setting: [3200K]
| [R GAIN] | Sets the correction level of red to the color temperature. [−400]…[+400] Factory setting: [0]
| [B GAIN] | Sets the correction level of blue to the color temperature. [−400]…[+400] Factory setting: [0]
| [G AXIS] | Sets the correction level of green to the color temperature. [−400]…[+400] Factory setting: [0]
[COLOR TEMP ACH/BCH] | — | When the camera is connected to the system, only [COLOR TEMP ACH] can be set.
| [COLOR TEMP ACH] | Sets the color temperature when the <WHITE BAL> switch is <A>. When the <CC> filter is set to <B><3200K>: [2000K]…[15000K] When the <CC> filter is set to <C><4300K>: [2300K]…[99999K] When the <CC> filter is set to <D><6300K>: [2700K]…[99999K] Factory setting: [3200K]
| [R GAIN ACH] | Sets the correction level of red to the color temperature. [−400]…[+400] Factory setting: [0]
| [B GAIN ACH] | Sets the correction level of blue to the color temperature. [−400]…[+400] Factory setting: [0]
| [G AXIS ACH] | Sets the correction level of green to the color temperature. [−400]…[+400] Factory setting: [0]
| [COLOR TEMP BCH] | Sets the color temperature when the <WHITE BAL> switch is <B>. When the <CC> filter is set to <B><3200K>: [2000K]…[15000K] When the <CC> filter is set to <C><4300K>: [2300K]…[99999K] When the <CC> filter is set to <D><6300K>: [2700K]…[99999K] Factory setting: [3200K]
| [R GAIN BCH] | Sets the correction level of red to the color temperature. [−400]…[+400] Factory setting: [0]
| [B GAIN BCH] | Sets the correction level of blue to the color temperature. [−400]…[+400] Factory setting: [0]
| [G AXIS BCH] | Sets the correction level of green to the color temperature. [−400]…[+400] Factory setting: [0]
[COLOR TEMP USER SW] | [COLOR TEMP] | Sets the color temperature when any of the <USER 1>/<USER 2>/<USER 3>/<USER 4> buttons are set to [C.TEMP] and the setting is enabled. When the <CC> filter is set to <B><3200K>: [2000K]…[15000K] When the <CC> filter is set to <C><4300K>: [2300K]…[99999K] When the <CC> filter is set to <D><6300K>: [2700K]…[99999K] Factory setting: [3200K]
| [R GAIN] | Sets the correction level of red to the color temperature. [−400]…[+400] Factory setting: [0]
| [B GAIN] | Sets the correction level of blue to the color temperature. [−400]…[+400] Factory setting: [0]
| [G AXIS] | Sets the correction level of green to the color temperature. [−400]…[+400] Factory setting: [0]

## [RGB GAIN CONTROL SETTING]

Item | Description of settings
--- | ---
[RGB GAIN ABS DISP SWITCH] | Sets whether to show the absolute value display for Ach/Bch inRGB gain. [OFF], [ON] Factory setting: [OFF]
[G GAIN REL CONTROL SWITCH] | Enables/disables the relative value control of Gch gain. [OFF], [ON] Factory setting: [OFF]
[RGB GAIN PRESET] | [R GAIN] | Sets the preset value of Rch gain. [−1000]…[+1000] Factory setting: [0]
| [G GAIN] | Sets the preset value of Gch gain. [−1000]…[+1000] Factory setting: [0]
| [B GAIN] | Sets the preset value of Bch gain. [−1000]…[+1000] Factory setting: [0]
[RGB GAIN ACH/BCH] | — | When the camera is connected to the CCU, only [R GAIN ACH]/[G GAIN ACH]/[B GAIN ACH]/[GAIN OFFSET ACH] can be set.
| [R GAIN ACH] | Sets the correction level of red to the gain. [−1000]…[+1000] Factory setting: [0]
| [G GAIN ACH] | Sets the correction level of green to the gain. [−1000]…[+1000] Factory setting: [0]
| [B GAIN ACH] | Sets the correction level of blue to the gain. [−1000]…[+1000] Factory setting: [0]
| [GAIN OFFSET ACH] | Sets whether to maintain the Rch, Gch, and Bch gain levels when adjusting the automatic white balance. [ON]: Maintains the values set in [R GAIN ACH], [G GAIN ACH], and [B GAIN ACH]. [OFF]: Sets [R GAIN ACH], [G GAIN ACH], and [B GAIN ACH] to [0]. Factory setting: [OFF]
| [R GAIN BCH] | Sets the correction level of red to the gain. [−1000]…[+1000] Factory setting: [0]
| [G GAIN BCH] | Sets the correction level of green to the gain. [−1000]…[+1000] Factory setting: [0]
| [B GAIN BCH] | Sets the correction level of blue to the gain. [−1000]…[+1000] Factory setting: [0]
| [GAIN OFFSET BCH] | Sets whether to maintain the Rch, Gch, and Bch gain levels when adjusting the automatic white balance. [ON]: Maintains the values set in [R GAIN BCH], [G GAIN BCH], and [B GAIN BCH]. [OFF]: Sets [R GAIN BCH], [G GAIN BCH], and [B GAIN BCH] to [0]. Factory setting: [OFF]

## [WHITE SHADING]

Item | Description of settings
--- | ---
[CORRECT] | Enables/disables the white shading (saw-toothed waveform or parabolic waveform) correction. [OFF], [ON] Factory setting: [ON]
[H SAW R] | Adjusts the white shading gain for Rch horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[H SAW G] | Adjusts the white shading gain for Gch horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[H SAW B] | Adjusts the white shading gain for Bch horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[H PARA R] | Adjusts the white shading gain for Rch horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[H PARA G] | Adjusts the white shading gain for Gch horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[H PARA B] | Adjusts the white shading gain for Bch horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[V SAW R] | Adjusts the white shading gain for Rch vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[V SAW G] | Adjusts the white shading gain for Gch vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[V SAW B] | Adjusts the white shading gain for Bch vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
[V PARA R] | Adjusts the white shading gain for Rch vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[V PARA G] | Adjusts the white shading gain for Gch vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]
[V PARA B] | Adjusts the white shading gain for Bch vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]

## [FLARE]

Item | Description of settings
--- | ---
[FLARE] | Enables/disables flare correction. [OFF], [ON] Factory setting: [ON]
[MASTER FLARE] | Adjusts the master flare. [−100]…[+100] Factory setting: [0]
[R FLARE] | Adjusts the Rch flare. [−100]…[+100] Factory setting: [0]
[G FLARE] | Adjusts the Gch flare. [−100]…[+100] Factory setting: [0]
[B FLARE] | Adjusts the Bch flare. [−100]…[+100] Factory setting: [0]

## [GAMMA/BLACK GAMMA]

Item | Description of settings
--- | ---
[GAMMA] | Enables/disables gamma correction. This cannot be set in HDR mode. [OFF], [ON] Factory setting: [ON]
[GAMMA MODE SELECT] | Selects the type of gamma. [HD], [FILMLIKE1], [FILMLIKE2], [FILMLIKE3], [FILM REC], [VIDEO REC] Factory setting: [HD]
[MASTER GAMMA] | Adjusts the gamma characteristic. When [GAMMA MODE SELECT] is [HD]: [0.150]…[0.750] (0.0020 step) When [GAMMA MODE SELECT] is [FILMLIKE1]/[FILMLIKE2]/[FILMLIKE3]: [0.3000]…[0.7500] (0.0025 step) When [GAMMA MODE SELECT] is [FILE REC]/[VIDEO REC]: [0.150]…[0.750] (0.0020 step) When [MAIN MENU]→[PAINT]→[DRS]→[DRS] is [ON]: [0.150]…[0.750] (0.0020 step) Factory setting: [0.450]
[R GAMMA] | Adjusts the gamma characteristic of red to the master gamma. [−75]…[+75] Factory setting: [0]
[B GAMMA] | Adjusts the gamma characteristic of blue to the master gamma. [−75]…[+75] Factory setting: [0]
[BLACK STRETCH LEVEL] | (Only when [FILM REC] is set) Sets the position of the gamma stretch. [0%]…[30%] Factory setting: [0%]
[DYNAMIC LEVEL] | (Only when [FILM REC] is set) Sets dynamic range. [200%], [300%], [400%], [500%] Factory setting: [500%]
[KNEE POINT] | (Only when [VIDEO REC] is set) Sets the knee point. [30]…[90] Factory setting: [30]
[KNEE SLOPE] | (Only when [VIDEO REC] is set) Sets the knee slope. [150%]/[200%]/[250%]/[300%]/[350%]/[400%]/[450%]/[500%]/[550%]/[600%] Factory setting: [150%]
[BLACK GAMMA] | Enables/disables black gamma. This cannot be set when [MAIN MENU] → [PAINT] → [DRS] → [DRS] → [ON] is set. [OFF], [ON] Factory setting: [OFF]
[MASTER BLACK GAMMA] | Adjusts the gamma characteristic adjacent to black. [−48]…[+48] Factory setting: [0]
[R BLACK GAMMA] | Adjusts the gamma characteristic of red adjacent to black to the master gamma. [−20]…[+20] Factory setting: [0]
[B BLACK GAMMA] | Adjusts the gamma characteristic of blue adjacent to black to the master gamma. [−20]…[+20] Factory setting: [0]
[INITIAL GAMMA] | Sets the gamma initial slope. When [GAMMA MODE SELECT] is [HD]: [4.0]/[4.5]/[5.0] When [GAMMA MODE SELECT] is [FILMLIKE1]/[FILMLIKE2]/[FILMLIKE3]: [4.5] (fixed) When [GAMMA MODE SELECT] is [FILE REC]/[VIDEO REC]: [4.5] (fixed) Factory setting: [4.5]

## [KNEE]

Item | Description of settings
--- | ---
[KNEE] | — | Enables/disables the knee function. This cannot be set in HDR mode. [OFF], [ON] Factory setting: [ON]
| [KNEE MASTER POINT] | Sets the knee point position. [080.00%]…[110.00%] (0.25% step) Factory setting: [95.00%]
| [KNEE R POINT] | Adjusts the knee point of red to [KNEE MASTER POINT]. [−25.00]…[25.00%] (0.25% step) Factory setting: [0.00%]
| [KNEE B POINT] | Adjusts the knee point of blue to [KNEE MASTER POINT]. [−25.00]…[25.00%] (0.25% step) Factory setting: [0.00%]
| [KNEE MASTER SLOPE] | Sets the knee slope. [00]…[199] Factory setting: [130]
| [KNEE R SLOPE] | Adjusts the knee slope of red to [KNEE MASTER SLOPE]. [−99]…[+99] Factory setting: [0]
| [KNEE B SLOPE] | Adjusts the knee slope of blue to [KNEE MASTER SLOPE]. [−99]…[+99] Factory setting: [0]

## [WHITE CLIP]

Item | Description of settings
--- | ---
[WHITE CLIP] | Enables/disables the white clip function. This cannot be set in HDR mode. [OFF], [ON] Factory setting: [ON]
[MASTER WHITE CLIP LEVEL] | Sets the white clip level. [80%]…[109%] Factory setting: [109%]
[R WHITE CLIP LEVEL] | Adjusts red to [MASTER WHITE CLIP LEVEL]. [−15%]…[+15%] Factory setting: [0%]
[B WHITE CLIP LEVEL] | Adjusts blue to [MASTER WHITE CLIP LEVEL]. [−15%]…[+15%] Factory setting: [0%]
[HI-COLOR] | Sets whether to improve the color reproduction in high-luminance areas. [OFF], [ON] Factory setting: [OFF]
[HI-COLOR LEVEL] | Sets the level of the mode that expands the color dynamic range. [1]…[32] Factory setting: [32]

## [DRS]

Item | Description of settings
--- | ---
[DRS] | Enables/disables the dynamic range stretcher function. Set this to [ON] to automatically adjust the contrast. This cannot be set in HDR mode. [OFF], [ON] Factory setting: [OFF]
[EFFECT DEPTH] | Sets the compression level of the high-luminance areas of the dynamic range stretcher function. Set a larger value to increase the compression level of the high-luminance areas. [1]…[5] Factory setting: [5]

## [DETAIL SETTING]

Item | Description of settings
--- | ---
[DETAIL] | Enables/disables all detail functions. [OFF], [ON] Factory setting: [ON]
[MASTER DETAIL] | Sets the master detail. [−31]…[+31] Factory setting: [0]
[H DETAIL LEVEL] | Sets the correction level of the horizontal detail. [00]…[63] Factory setting: [15]
[V DETAIL LEVEL] | Sets the correction level of the vertical detail. [00]…[63] Factory setting: [20]
[PEAK FREQUENCY] | Sets the peak frequency of the horizontal detail. [12.4MHz], [12.5MHz], [12.7MHz], [12.9MHz], [13.0MHz], [13.3MHz], [13.6MHz], [13.9MHz], [14.2MHz], [14.6MHz], [15.0MHz], [15.5MHz], [16.1MHz], [16.7MHz], [17.3MHz], [18.3MHz], [18.6MHz], [18.8MHz], [19.0MHz], [19.2MHz], [19.5MHz], [19.9MHz], [20.3MHz], [20.9MHz], [21.5MHz], [22.4MHz], [23.6MHz], [25.4MHz], [28.6MHz], [37.1MHz] Factory setting: [19.0MHz]
[V DETAIL FREQUENCY] | Sets the vertical detail frequency. [00]…[31] Factory setting: [18]
[CRISP] | Sets the detail signal noise removal level. [00]…[63] Factory setting: [0]
[DETAIL GAIN(+)] | Sets the detail level in the + (upward) direction. [−31]…[+31] Factory setting: [0]
[DETAIL GAIN(−)] | Sets the detail level in the − (downward) direction. [−31]…[+31] Factory setting: [0]
[DETAIL CLIP+] | Adjust the detail clip to reduce glare produced by an excess of details. [00]…[63] Factory setting: [0]
[DETAIL CLIP−] | Adjusts the length of the undershoot of the detail edge component. [00]…[63] Factory setting: [0]
[DETAIL SOURCE] | Sets the RGB signal component ratio to create the detail. [(G+R)/2], [(G+B)/2], [(2G+B+R)/4], [(3G+R)/4], [R], [G] Factory setting: [(G+R)/2]
[KNEE APERTURE LEVEL] | Adjusts the knee aperture level. This cannot be set in HDR mode. [00]…[39] Factory setting: [5]
[DETAIL KNEE] | Adjusts the detail components of knee. [00]…[15] Factory setting: [0]
[LEVEL DEPENDENT SWITCH] | Enables/disables the function to remove details of dark areas. This cannot be set in HDR mode. [OFF], [ON] Factory setting: [OFF]
[LEVEL DEPENDENT] | Sets the level to remove details of dark areas. [00]…[15] Factory setting: [8]
[DARK DETAIL SWITCH] | Enables/disables the function to emphasize details of dark areas. This cannot be set in HDR mode. [OFF], [ON] Factory setting: [OFF]
[DARK DETAIL] | Sets the level to emphasize details of dark areas. [00]…[7] Factory setting: [3]

## [SKIN TONE DETAIL SETTING]

Item | Description of settings
--- | ---
[SKIN TONE DETAIL] | Enables/disables the skin tone detail function. This cannot be set if [MAIN MENU] → [PAINT] → [DETAIL SETTING] → [DETAIL] → [OFF] is set. [OFF], [ON] Factory setting: [OFF]
[SKIN GET] | — | Selects whether to automatically obtain the color saturation and hue information from the cursor position. [NO], [YES]
| [MEMORY SELECT] | Selects the skin tone table of the subject to apply the skin tone table to. [A], [B], [C] Factory setting: [A]
| [CURSOR] | Shows/hides the box cursor in the center of the screen. [OFF], [ON] Factory setting: [OFF]
| [H POSITION] | Adjusts the horizontal position of the cursor. [0%]…[100%] (0.25% step) Factory setting: [50%]
| [V POSITION] | Adjusts the vertical position of the cursor. [0%]…[100%] (0.25% step) Factory setting: [50%]
[ZEBRA] | — | Enables/disables the zebra display. [OFF], [ON] Factory setting: [OFF]
| [ZEBRA EFFECT MEMORY] | Selects the table of the zebra display. [A], [B], [C], [A+B], [A+C], [B+C], [A+B+C] Factory setting: [A+B+C]
[SKIN TONE EFFECT MEMORY] | Selects the skin tone table used to apply the skin tone detail. [A], [B], [C], [A+B], [A+C], [B+C], [A+B+C] Factory setting: [A+B+C]
[SKIN TONE CRISP] | Adjusts the skin tone detail. [−63]…[+63] Factory setting: [+63]
[I CENTER] | Sets the center position on the I axis (the area where the skin tone effect is applied). [0]…[255] Factory setting: [33]
[I WIDTH] | Sets the width of the area where the skin tone effect is applied on the I axis with [I CENTER] being the center. [0]…[255] Factory setting: [10]
[Q WIDTH] | Sets the width of the area where the skin tone effect is applied on the Q axis with [I CENTER] being the center. [0]…[255] Factory setting: [28]
[Q PHASE] | Sets the phase of the area where the skin tone effect is applied with the Q axis being the reference. [0]…[359] Factory setting: [89]

## [LINEAR MATRIX]

Item | Description of settings
--- | ---
[PRESET MATRIX] | Sets the preset matrix. [NORM], [EBU], [NTSC] Factory setting: [NORM]
[MATRIX] | Enables/disables the matrix function. [OFF], [ON] Factory setting: [OFF]
[LINEAR MATRIX] | — | Enables/disables the linear matrix function. [OFF], [ON] Factory setting: [OFF]
| [LINEAR TABLE] | Selects the table for linear matrix. [A], [B] Factory setting: [A]
[COLOR CORRECT] | — | Enables/disables the 12-axis color correction function. [OFF], [ON] Factory setting: [OFF]
| [COLOR CORRECT TABLE] | Selects the table for color correction. [A], [B] Factory setting: [A]
[MATRIX (R-G)_N] | Adjusts the linear matrix between red and green. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (R-G)_P] | Adjusts the linear matrix between red and green. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (R-B)_N] | Adjusts the linear matrix between red and blue. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (R-B)_P] | Adjusts the linear matrix between red and blue. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (G-R)_N] | Adjusts the linear matrix between green and red. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (G-R)_P] | Adjusts the linear matrix between green and red. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (G-B)_N] | Adjusts the linear matrix between green and blue. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (G-B)_P] | Adjusts the linear matrix between green and blue. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (B-R)_N] | Adjusts the linear matrix between blue and red. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (B-R)_P] | Adjusts the linear matrix between blue and red. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (B-G)_N] | Adjusts the linear matrix between blue and green. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]
[MATRIX (B-G)_P] | Adjusts the linear matrix between blue and green. This item is not available when [MATRIX] is set to [OFF]. [−31]…[+31] Factory setting: [0]

## [COLOR CORRECTION]

Item | Description of settings
--- | ---
[PRESET MATRIX] | Sets the preset matrix. [NORM], [EBU], [NTSC] Factory setting: [NORM]
[MATRIX] | Enables/disables the matrix function. [OFF], [ON] Factory setting: [OFF]
[LINEAR MATRIX] | — | Enables/disables the linear matrix function. [OFF], [ON] Factory setting: [OFF]
| [LINEAR TABLE] | Selects the table for linear matrix. [A], [B] Factory setting: [A]
[COLOR CORRECT] | — | Enables/disables the 12-axis color correction function. [OFF], [ON] Factory setting: [OFF]
| [COLOR CORRECT TABLE] | Selects the table for color correction. [A], [B] Factory setting: [A]
[G SAT] | Adjusts green color saturation. [−127]…[+126] Factory setting: [0]
[G_CY SAT] | Adjusts the color saturation between green and cyan. [−127]…[+126] Factory setting: [0]
[CY SAT] | Adjusts cyan color saturation. [−127]…[+126] Factory setting: [0]
[CY_B SAT] | Adjusts the color saturation between cyan and blue. [−127]…[+126] Factory setting: [0]
[B SAT] | Adjusts blue color saturation. [−127]…[+126] Factory setting: [0]
[B_MG SAT] | Adjusts the color saturation between blue and magenta. [−127]…[+126] Factory setting: [0]
[MG_SAT] | Adjusts magenta color saturation. [−127]…[+126] Factory setting: [0]
[MG_R SAT] | Adjusts the color saturation between magenta and red. [−127]…[+126] Factory setting: [0]
[R SAT] | Adjusts red color saturation. [−127]…[+126] Factory setting: [0]
[R_YE SAT] | Adjusts the color saturation between red and yellow. [−127]…[+126] Factory setting: [0]
[YE SAT] | Adjusts yellow color saturation. [−127]…[+126] Factory setting: [0]
[YE_G SAT] | Adjusts the color saturation between yellow and green. [−127]…[+126] Factory setting: [0]
[G PHASE] | Adjusts green hue. [−127]…[+127] Factory setting: [0]
[G_CY PHASE] | Adjusts the hue between green and cyan. [−127]…[+127] Factory setting: [0]
[CY PHASE] | Adjusts cyan hue. [−127]…[+127] Factory setting: [0]
[CY_B PHASE] | Adjusts the hue between cyan and blue. [−127]…[+127] Factory setting: [0]
[B PHASE] | Adjusts blue hue. [−127]…[+127] Factory setting: [0]
[B_MG PHASE] | Adjusts the hue between blue and magenta. [−127]…[+127] Factory setting: [0]
[MG_PHASE] | Adjusts magenta hue. [−127]…[+127] Factory setting: [0]
[MG_R PHASE] | Adjusts the hue between magenta and red. [−127]…[+127] Factory setting: [0]
[R PHASE] | Adjusts red hue. [−127]…[+127] Factory setting: [0]
[R_YE PHASE] | Adjusts the hue between red and yellow. [−127]…[+127] Factory setting: [0]
[YE PHASE] | Adjusts yellow hue. [−127]…[+127] Factory setting: [0]
[YE_G PHASE] | Adjusts the hue between yellow and green. [−127]…[+127] Factory setting: [0]
[COLOR CORRECTION GET] | — | Obtains the color information automatically from the cursor position and moves the menu arrow to the axis whose color is to be adjusted. [NO], [YES]
| [CURSOR] | Shows/hides the box cursor in the center of the screen. [OFF], [ON] Factory setting: [OFF]
| [H POSITION] | Adjusts the horizontal position of the cursor. [0%]…[100%] (0.25% step) Factory setting: [50%]
| [V POSITION] | Adjusts the vertical position of the cursor. [0%]…[100%] (0.25% step) Factory setting: [50%]

## [SKIN CORRECTION]

Item | Description of settings
--- | ---
[SKIN AREA SW] | Enables/disables the function to finely adjust the color of the skin tone area. [OFF], [ON] Factory setting: [OFF]
[SKIN AREA TABLE] | Selects the table for the skin tone area. [A], [B] Factory setting: [A]
[SKIN AREA HUE] | Finely adjusts the hue of the skin tone area. [−127]…[+127] Factory setting: [0]
[SKIN AREA TONE] | Finely adjusts the tone of the skin tone area. [−127]…[+126] Factory setting: [0]

## [DNR]

Item | Description of settings
--- | ---
[DNR SW] | Enables/disables the noise reduction function. [OFF], [ON] Factory setting: [OFF]
[DNR LEVEL] | Sets the level of noise reduction. [1]…[5] Factory setting: [3]

## [SCENE FILE]

Item | Description of settings
--- | ---
[MODE] | Selects the operation mode. [LOAD], [STORE] Factory setting: [LOAD]
[FILE NO.] | Selects a file number. When [MODE] is [LOAD]: [OFF], [1]…[8] When [MODE] is [STORE]: [1]…[8] Factory setting: [1]
[FILE NAME] | Enters a file name. (15 characters or less) Factory setting: [SCENE1]
[EXECUTE] | Selects whether to execute with the configured settings. [NO], [YES]

## [ROP CONTROL]

Item | Description of settings
--- | ---
[CONTROL ROTATION MODE] | Sets the control rotation mode of ROP. [MODE1], [MODE2] Factory setting: [MODE2]

Top of the page