- Top
- Maintenance
- Warning displays
- Camera warning displays

# Camera warning displays

#### When AWB (automatic white balance) is executed

[AWB BREAK] | Automatic white balance has been interrupted.
[AWB HIGH LIGHT NG] | Automatic white balance cannot be executed because the light amount is excessive. Set the light amount to an appropriate level.
[AWB LOW LIGHT NG] | Automatic white balance cannot be executed because the light amount is insufficient. Set the light amount to an appropriate level.
[AWB NG CHECK FILTER] | Automatic white balance cannot be executed because of erroneous filter position. Set the correct filter position.
[AWB RCH OUT RANGE] | The white balance convergence for red cannot be achieved. Shoot a uniformly white object on the screen, and execute AWB.
[AWB BCH OUT RANGE] | The white balance convergence for blue cannot be achieved. Shoot a uniformly white object on the screen, and execute AWB.

#### When ABB (automatic black balance) is executed

[ABB BREAK] | Automatic black balance has been interrupted.
[ABB RCH OUT RANGE] | The black balance convergence for red cannot be achieved. Check if there are any errors in the image.
[ABB BCH OUT RANGE] | The black balance convergence for blue cannot be achieved. Check if there are any errors in the image.
[ABB GCH OUT RANGE] | The black balance convergence for green cannot be achieved. Check if there are any errors in the image.
[ABB NG] | The lens iris may not be closed.

#### Executing black shading

[BSHD] | Black shading is executing.
[BSHD BRAK] | Black shading has been interrupted.
[BSHD NG] | An error has occurred with the black shading. Check if the lens is correctly closed.

#### When ASU (automatic setup) is executed

[AUTO SETUP BREAK] | Automatic setup has been interrupted.
[ASU NG] [LENS CTL NG OUT RANGE] | The lens iris control cannot be performed. Check the lens settings.
[ASU NG] [AWB RCH NG] | An error in red has occurred. Check the white balance settings.
[ASU NG] [AWB BCH NG] | An error in blue has occurred. Check the white balance settings.
[ASU NG] [ABB RCH NG] | An error in red has occurred. Check the black balance settings.
[ASU NG] [ABB BCH NG] | An error in blue has occurred. Check the black balance settings.
[ASU NG] [ABB GCH NG] | An error in green has occurred. Check the black balance settings.
[ASU NG] [BSHD RCH NG] | An error in red has occurred. Adjust black shading.
[ASU NG] [BSHD BCH NG] | An error in blue has occurred. Adjust black shading.
[ASU NG] [BSHD GCH NG] | An error in green has occurred. Adjust black shading.
[ASU NG] [BSHD BREAK] | Black shading has been interrupted.
[ASU NG] [BSHD NG] | An error in black shading has occurred.
[ASU NG] [GAMMA RCH NG] | An error in red has occurred. Check the gamma settings.
[ASU NG] [GAMMA BCH NG] | An error in blue has occurred. Check the gamma settings.
[ASU NG] [FLARE RCH NG] | An error in red has occurred. Check the flare settings.
[ASU NG] [FLARE BCH NG] | An error in blue has occurred. Check the flare settings.
[ASU NG] [ABB MPED NG] | An error in master pedestal has occurred. Check the master pedestal settings of automatic black balance.
[ASU NOT RUNNING(BAR)] | Automatic setup is prohibited.
[ASU NOT RUNNING(TEST)] | Automatic setup is prohibited.
[ASU NOT RUNNING(D.EXT)] | Automatic setup is prohibited.
[ASU NOT RUNNING(HDR)] | Automatic setup is prohibited.

Top of the page