- Top
- Menu Operations
- Menu list
- [IN/OUT SELECT]

# [IN/OUT SELECT]

Item | Description of settings
--- | ---
[CALL TALLY] | Sets whether the rear tally lamp is to be lit up when called. [OFF]: Turned off. [R]: Red tally lights up. [T]: Up tally lights up. [R&T]: Red tally and up tally light up. Factory setting: [OFF]
[TALLY GUARD] | Enables/disables automatic white balance, automatic black balance, and automatic setup when the tally lamp is lit. [OFF], [ON] Factory setting: [OFF]
[HD-SDI1 OUT] | Configures the video output from the <HD SDI1> terminal. [CAM]: Outputs camera images. [HD PROMPT]: Outputs HD prompter video images. Factory setting: [CAM]
[HD-SDI1 OUTPUT FORMAT] | Sets the signal format of the video output from the <HD SDI1> terminal. [1080i], [1080P], [720P] Factory setting: [1080i]
[HD-SDI1 OUTPUT ITEM] | Selects details of the characters superimposed on images output from the <HD SDI1> terminal. [MENU ONLY]: Displays only on the menu. [STATUS]: Displays all characters that are the same as in the viewfinder display. Factory setting: [MENU ONLY]
[HD-SDI1 CHAR] | Sets whether to superimpose characters on images output from the <HD SDI1> terminal. This cannot be set when the output format is [720P]. [OFF], [ON] Factory setting: [OFF]
[HD-SDI1 CHAR SIZE] | Sets the size of the characters superimposed on images output from the <HD SDI1> terminal. [LARGE], [SMALL] Factory setting: [SMALL]
[HD-SDI1 3G-SDI] | Sets the output format when the video output from the <HD SDI1> terminal is in 3G format. [LEVEL-A], [LEVEL-B] Factory setting: [LEVEL-A]
[HD-SDI2 OUT] | Configures the video output from the <HD SDI2> terminal. [CAM]: Outputs camera images. [VF]: Outputs viewfinder images. [RET]: Outputs return images. [RET1], [RET2], [RET3], [RET4]: Outputs fixed return images. Factory setting: [VF]
[HD-SDI2 OUTPUT FORMAT] | Sets the signal format of the video output from the <HD SDI2> terminal. [1080i], [1080P], [720P] Factory setting: [1080i]
[HD-SDI2 OUTPUT ITEM] | Selects details of the characters superimposed on images output from the <HD SDI2> terminal. [MENU ONLY]: Displays only on the menu. [STATUS]: Displays all characters that are the same as in the viewfinder display. Factory setting: [MENU ONLY]
[HD-SDI2 CHAR] | Sets whether to superimpose characters on images output from the <HD SDI2> terminal. This cannot be set when the output format is [720P]. [OFF], [ON] Factory setting: [OFF]
[HD-SDI2 CHAR SIZE] | Selects the size of the characters superimposed on images output from the <HD SDI2> terminal. [LARGE], [SMALL] Factory setting: [SMALL]
[HD-SDI2 3G-SDI] | Sets the output format when the video output from the <HD SDI2> terminal is in 3G format. [LEVEL-A], [LEVEL-B] Factory setting: [LEVEL-A]
[HD-SDI2 POWER] | Enables/disables the power supply of the <HD SDI2> terminal. [ACTIVE], [SAVE] Factory setting: [ACTIVE]
[AUX I/O] | Configures the video output from the <AUX> terminal. [PMT2 OUT], [HD TRUNK] Factory setting: [PMT2 OUT]
[VF OUT] | Configures the video output from the <VF> terminal. [Y/C], [R], [G], [B], [NAM] Factory setting: [ENC]
[TRUNK1] | Sets the serial interface standard of the <TRUNK> terminal. [RS422], [RS232C] Factory setting: [RS422]
[TRUNK2] | Sets the serial interface standard of the <TRUNK> terminal. [RS422], [RS232C] Factory setting: [RS422]
[BACK LIGHT] | Sets the brightness of the backlight. [1]…[70] Factory setting: [20]
[LAN] | Sets the usage for the <LAN> terminal. [TRUNK], [PC] Factory setting: [PC]
[B/U LENS] | Sets the lens type of the Build-up Unit. [PORTABLE], [BOX] Factory setting: [BOX]
[T-BAR CONNECT] | Sets whether to connect the T-BAR unit. [OFF], [ON] Factory setting: [OFF]
[LENS I/F] | Sets the lens interface. [ANALOG], [SERIAL] Factory setting: [SERIAL]
[DISPLAY STATUS/BAR OSD] | [CAM ID CHARACTER] | Sets the camera name.
[GEN-LOCK] | [H PHASE-COARSE] | Roughly adjusts the phase of horizontal synchronization. [−5]…[+5] Factory setting: [0]
| [H PHASE-FINE] | Finely adjusts the phase of horizontal synchronization. [−100]…[+100] Factory setting: [0]

Top of the page