- Top
- Specifications
- Details of the connector signals

# Details of the connector signals

OPT FIBER
| 1 | OPT-TX(Mark Band=IN)
2 | OPT-RX(Mark Band=OUT)
3 | AC240V(C)
4 | AC240V(H)
5 | STBY-SIG
6 | STBY-CONT
TAJIMI ELECTRONICS
| 1 | OPT-TX(Mark Band=IN)
2 | OPT-RX(Mark Band=OUT)
3 | STBY-SIG
4 | STBY-CONT
5 | AC240V(C)
6 | AC240V(H)
LEMO

INTERCOM
| 1 | TALK GND
2 | TALK
3 | RECEIVE GND
4 | RECEIVE CH1
5 | RECEIVE CH2
HA16PRH-5S (Hirose Electric Co.)

RET CTRL
| 1 | INTERCOM1 MIC ON
2 | INTERCOM2 MIC ON
3 | GND
4 | RET CONT3
5 | RET CONT1
6 | RET CONT2
HR10A-10R-10SB(71) (Hirose Electric Co.)

DC IN
| 1 | UNREG GND
2 | Not used
3 | Not used
4 | +12 V
HA16RA-4P(77) (Hirose Electric Co.)

EXT IO
| 1 | CRANE DATA(H)
2 | CRANE DATA(C)
3 | CRANE CONT(H)
4 | CRANE CONT(C)
5 | GND
6 | CRANE INTERCOM RECEIVE
7 | CRANE INTERCOM RECEIVE GND
8 | CRANE INTERCOM TALK
9 | CRANE INTERCOM TALK GND
10 | CRANE PGM1 LEVEL
11 | CRANE PGM2 LEVEL
12 | Not used
13 | Not used
14 | G TALLY VF
15 | R TALLY VF
16 | T TALLY VF
17 | CRANE ACT
18 | UNREG +12 V
19 | Not used
20 | UNREG GND
HR10A-13R-20SC (Hirose Electric Co.)

REMOTE
| 1 | CAM DATA (H)
2 | CAM DATA (C)
3 | CAM CONT(H)
4 | CAM CONT(C)
5 | Not used
6 | Not used
7 | Not used
8 | Not used
9 | UNREG +12 V
10 | UNREG GND
HR10A-10R-10SC (Hirose Electric Co.)

MIC (front)
| 1 | GND
2 | AUDIO IN (H)
3 | AUDIO IN (C)
HA16PRM-3SG (Hirose Electric Co.)

MIC (rear)
| 1 | GND
2 | AUDIO IN (H)
3 | AUDIO IN (C)
HA16PRM-3SG (Hirose Electric Co.)

DC OUT 1.0A
| 1 | GND
2 | R TALLY (open collector)
3 | G TALLY (open collector)
4 | UNREG +12 V (max. 1.0 A)
HR10A-7R-4SC (Hirose Electric Co.)

EARPHONE
— | 1 | GND
2 | AUDIO OUT1
3 | AUDIO OUT2

TRUNK
| 1 | CMD OUT0(H)
2 | CMD OUT0(C)
3 | CMD IN0(H)
4 | CMD IN0(C)
5 | CMD OUT1(H)
6 | CMD OUT1(C)
7 | CMD IN1(H)
8 | CMD IN1(C)
9 | Not used
10 | GND
11 | Not used
12 | Not used
HR10A-10R-12SC (Hirose Electric Co.)

LENS
| 1 | RET-SW
2 | REC
3 | GND
4 | IRIS-AUTO
5 | IRIS-CONT
6 | UNREG +12 V
7 | IRIS-POSI
8 | IRIS-G-MAX
9 | EXT-POSI
10 | ZOOM-POSI
11 | FOCUS POSI/LENS RXD
12 | IRIS AUTO/LENS TXD
HR10A-10R-12SC (Hirose Electric Co.)

VF (front)
| 1 | UNREG-12V
2 | UNREG-12V
3 | +9 V
4 | VF-PB-OUT-GND
5 | VF-PR-OUT-GND
6 | VF-Y-OUT
7 | VF-Y-OUT-GND
8 | VF-CLK
9 | VF-WR
10 | VF-DATA
11 | UNREG-GND
12 | ZEBRA-SW
13 | PEAKING
14 | TA BOX ACT
15 | VF-PB-OUT
16 | VF-PR-OUT
17 | VF-SW3
18 | FRONT-VR
19 | TA TALLY
20 | GND
HR12-14RF-20SDL (Hirose Electric Co.)

VF (rear)
| 1 | VF-Y-OUT
2 | VF-PB-OUT
3 | VF-PR-OUT
4 | CAM DETECT
5 | I2C DATA
6 | R TALLY
7 | T TALLY
8 | UNREG +12 V
9 | UNREG +12 V
10 | UNREG +12 V
11 | VF-Y-OUT-GND
12 | VF-PB-OUT-GND
13 | VF-PR-OUT-GND
14 | AGND
15 | DGND
16 | Not used
17 | UNREG GND
18 | Not used
19 | FGND
20 | LCD ACT (Not used)
21 | Not used
22 | Not used
23 | PEAKING CONT (Not used)
24 | I2C CLK
25 | G TALLY
26 | VF P REQ
27 | RESERVED
28 | RESERVED
29 | RESERVED
D02F-29SF-N-F0 (Japan Aviation Electronics Industry)

BUILD UP
| 1 | Not used
2 | VF-PB-OUT-GND
3 | VF-PB-OUT
4 | VF-PR-OUT-GND
5 | VF-PR-OUT
6 | VF-Y-OUT
7 | VF-Y-OUT-GND
8 | CAM DATA
9 | CAM CONT
10 | Not used
11 | AC(H)
12 | Not used
13 | IRIS POS
14 | GND
15 | IRIS CNT
16 | FOCUS POS/L2C DATA
17 | C2L DATA
18 | BU ACT
19 | Not used
20 | AC(C)
QR/P8-20S-C (Hirose Electric Co.)

DC OUT 2.5A
| 1 | UNREG +12 V
2 | UNREG GND
VJS4444 (Panasonic)

Top of the page