- Top
- Specifications
- Specifications
- Specifications

# Specifications

## General

Power DC 12 V (when using an external power supply) AC 240 V, 50 Hz/60 Hz (when AK-UCU500P/AK-UCU500PS/AK-UCU500E/AK-UCU500ES is connected) Power consumption 119 W (maximum, when connecting to an external 12 V and including supply to an externally connected devices) 360 W (maximum, when AK-UCU500P/AK-UCU500PS/AK-UCU500E/AK-UCU500ES is conncected and including supply to an externally connected devices)

indicates safety information.

Ambient operating temperature | −10 °C – 45 °C (14 °F – 113 °F) (Preheating required under a temperature 0 °C (32 °F) or below)
Storage temperature | −20 °C – 60 °C (−4 °F – 140 °F)
Ambient operating humidity | 85% or less (relative humidity)
Weight | Approx. 4.4 kg (9.70 lbs.) (body only, excluding the accessories)
Dimensions (W×H×D) | Body only 151 mm × 267 mm × 371.5 mm (5-31/32 inches × 10-17/32 inches × 14-21/32 inches) (excluding protrusions)

## Camera unit

Pickup device | 2/3-type, 2.2 million pixels, MOS × 3
Optical filter | CC: 3200 K, 4300 K, 6300 K, Cross, Diffusion ND: CAP, Clear, 1/4, 1/16, 1/64
Lens mount | 2/3-type bayonet
Sensitivity | Two shooting modes [HIGH SENS]: F11 (59.94 Hz)/F12 (50 Hz) [NORMAL]: F8 (59.94 Hz)/F9 (50 Hz) 2000 lx, 3200 K, when white reflectivity is 89.9%
Horizontal modulation | 50% or above (27.5 MHz)
S/N | 60 dB or above
Horizontal resolution | 1000 TV lines or above (center)
Gain switching | [NORMAL]: −3, 0, 3, 6, 9, 12, 15, 18, 21, 24, 27, 30, 33, 36 [HIGH SENS]: −6, −3, 0, 3, 6, 9, 12, 15, 18, 21, 24, 27, 30, 33, 36
Shutter speed | [59.94i]/[59.94p] mode: 1/100, 1/120, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [29.97p] mode: 1/48, 1/50, 1/60, 1/96, 1/100, 1/120, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [23.98p] mode: 1/48, 1/50, 1/60, 1/96, 1/100, 1/120, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [50i]/[50p] mode: 1/60, 1/100, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [25p] mode: 1/48, 1/50, 1/60, 1/96, 1/100, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [200fps]/[240fps] mode: 1/250, 1/500, 1/1000, 1/1500, 1/2000

## Video input/output

<HD SDI1> terminal | BNC × 1 HD (3G/1.5G): 0.8 V [p-p], 75 Ω
<HD SDI2> terminal | BNC × 1 HD (3G/1.5G): 0.8 V [p-p], 75 Ω
<AUX> terminal | BNC × 1 Functions as <HD TRUNK> terminal/<PROMPTER2> terminal by switching the setting in the menu <HD TRUNK>: HD (1.5G) <PROMPTER2>: VBS signal 1 V [p-p], 75 Ω
<G/L IN/PROMPTER OUT> terminal | BNC × 1 <G/L IN>: Tri-level SYNC or black burst <PROMPTER OUT>: VBS signal 1 V [p-p], 75 Ω Functions as <G/L IN> when standalone, and as <PROMPTER OUT> when AK-UCU500P/AK-UCU500PS/AK-UCU500E/AK-UCU500ES is connected

## Audio input/output

<MIC 1> terminal | XLR × 1, 3-pin <LINE>/<MIC>/<+48V> switchable For <MIC>, <FRONT>/<REAR> switchable <LINE>: 0 dBu, +4 dBu menu selection available <MIC>: −60 dBu, −40 dBu, or −20 dBu menu can be selected
<MIC 2> terminal | XLR × 1, 3-pin <LINE>/<MIC>/<+48V> switchable <LINE>: 0 dBu, +4 dBu menu selection available <MIC>: −60 dBu, −40 dBu, or −20 dBu menu can be selected
<MIC> terminal (front) | XLR × 1, 3-pin Switchable with <MIC 1> terminal

## Intercom

<INTERCOM1> terminal | XLR × 1, 5-pin
<INTERCOM2> terminal | XLR × 1, 5-pin
<EARPHONE> terminal | Stereo mini jack × 1, 3-pin

## Other input/output

<OPT FIBER> terminal | Optical composite connector × 1
<LENS> terminal | 12-pin × 1
<VF> terminal | 20-pin × 1
<VF> terminal (rear) | 29-pin × 1
<DC IN> terminal | XLR × 1, 4-pin, DC 12 V
<DC OUT 12V 1A> terminal | 4-pin × 1
<RET CTRL> terminal | 6-pin × 1
<EXT I/O> terminal | 20-pin × 1, DC 12 V, 0.5 A
<REMOTE> terminal | 10-pin × 1
<TRUNK> terminal | 12-pin × 1
<DC OUT 12V 2.5A> terminal | 2-pin × 1
<LAN> terminal | RJ-45 × 1
<USB2.0> terminal (host) | Type A connector, DC 5 V, 0.5 A
Build-up terminal | 20-pin × 1

Top of the page