- Top
- Preparation
- Attaching the viewfinder
- Attaching the rear viewfinder

# Attaching the rear viewfinder

LCD viewfinder AK-HVF100G (optional) can be used with this camera.

For details on handling the LCD viewfinder, refer to the Operating Instructions of the viewfinder.

Connector cover

V-groove

Lock release button

V-shaped protrusion

Fig. 1

Fig. 2

Turn off the power of the camera and the LCD viewfinder.

Press the lock release button and remove the connector cover. (Fig. 1)

Align the V-shaped protrusion of the LCD viewfinder with the V-shaped groove on the camera and slide it in until the lock is engaged. (Fig. 2)

NOTE

- When attaching the viewfinder, refrain from holding the hood of the LCD viewfinder.

## Removing the rear viewfinder

Turn off the power of the camera and the LCD viewfinder.

While pressing the lock release button, slide off the LCD viewfinder.

NOTE

- When removing the viewfinder, refrain from holding the hood of the LCD viewfinder.

Top of the page