- Top
- Preparation
- Connecting a microphone
- When mounting a microphone on the viewfinder (optional) for use

# When mounting a microphone on the viewfinder (optional) for use

A microphone such as microphone kit AJ-MC700P (optional) can be mounted on the viewfinder.

Microphone holder

Clamp screw

Fig. 1

Fig. 2

<MIC 1> terminal

Fig. 3

Open the microphone holder. (Fig. 1)

Mount the microphone and tighten the clamp screw. (Fig. 2)

Insert the microphone cable into the cable clamp and connect it to the <MIC 1> terminal (front). (Fig. 3)

Set the <FRONT>/<REAR> switch (<MIC 1>) to <FRONT>.

Set the <LINE/MIC/+48V> selector switch (<MIC 1>) to <MIC> or <+48V>.

Top of the page