- Top
- Menu Operations
- Menu list
- [MIC SETTING]

# [MIC SETTING]

Item | Description of settings
--- | ---
[MIC1 GAIN] | Sets the gain when there is a microphone input to the <MIC 1> terminal. [60dB], [40dB], [20dB] Factory setting: [60dB]
[MIC1 LINE INPUT LEVEL] | Sets the input level when there is a line input to the <MIC 1> terminal. [0dB], [+4dB] Factory setting: [0dB]
[MIC1 AMP] | Adjusts the level of the input to the <MIC 1> terminal. [−20dB]…[+20dB] Factory setting: [0dB]
[MIC2 GAIN] | Sets the gain when there is a microphone input to the <MIC 2> terminal. [60dB], [40dB], [20dB] Factory setting: [60dB]
[MIC2 LINE INPUT LEVEL] | Sets the input level when there is a line input to the <MIC 2> terminal. [0dB], [+4dB] Factory setting: [0dB]
[MIC2 AMP] | Adjusts the level of the input to the <MIC 2> terminal. [−20dB]…[+20dB] Factory setting: [0dB]
[MIC2 INPUT SELECT] | Sets the input signal for the <MIC 2> terminal. This item can be set only when the PGM option is used. [FRONT MIC], [OFF] Factory setting: [OFF]
[FRONT MIC POWER] | Enables/disables the phantom power (48 V) for the external microphone connected to the <MIC> terminal (front). [ON], [OFF] Factory setting: [OFF]

Top of the page