- Top
- Description of Parts
- Upper side

# Upper side

1. Viewfinder front/back positioning lever

   To adjust the front/back position of the viewfinder, loosen this lever and slide the viewfinder forwards or backwards to adjust the viewfinder to a position that enables easy viewing. After adjusting the viewfinder, turn the lever towards <LOCK> to lock the position.

2. Viewfinder left-right positioning ring

   To adjust the left/right position of the viewfinder, loosen this lever and slide the viewfinder to the left or right to adjust the viewfinder to a position that enables easy viewing. Tighten the lever to clamp the viewfinder in place after adjusting.

3. Light shoe

   Used to mount a video light, etc.

4. Microphone holder holes

   Used to mount a microphone.

5. <PTT> switch

   Used to switch the intercom microphone on/off. The function can be changed in [MAIN MENU] → [SWITCH MODE] → [USER SWITCH] → [GRIP PTT].

6. <RET> switch

   Used to switch to the return A signal. The function can be changed in [MAIN MENU] → [SWITCH MODE] → [USER SWITCH] → [GRIP RET].

7. Accessory mounting hole

   Used to attach accessories. This hole is used only for the purpose of attaching accessories.

   - Mounting hole size

     - 1/4-20 UNC (screw length 13 mm or shorter)

8. Lock release button

   Used to release the lock of the V-groove.

9. V-groove

   Used to attach the rear viewfinder.

Top of the page