- Top
- Preparation
- Attaching the viewfinder
- Attaching the viewfinder

# Attaching the viewfinder

HD viewfinder AJ-HVF21KG (optional) can be used with this camera.

For details on handling the HD viewfinder, refer to the Operating Instructions of the viewfinder.

Viewfinder left-right positioning ring

Knob

Fig. 1

Fig. 2

Set the <POWER> switch to <OFF>.

Pull up the knob on the mounting plate and slide the plate to attach the viewfinder. (Fig. 1)

Securely tighten the viewfinder left-right positioning ring. (Fig. 1)

Connect the plug to the <VF> terminal. (Fig. 2)

NOTE

- When connecting the plug to the <VF> terminal, confirm that the plug is fully inserted in the terminal.

## Removing the viewfinder

Set the <POWER> switch to <OFF>.

Remove the plug from the <VF> terminal.

Loosen the viewfinder clamping dial and then pull up the knob on the mounting plate.

Slide the viewfinder along the plate to remove it from the plate.

Top of the page