- Top
- Overview
- Using the camera in a system
- Basic configuration devices

# Basic configuration devices

The basic system configuration includes the lens, Studio Handy Camera, viewfinder, Camera Control Unit (CCU), and Remote Operation Panel (ROP).

Part name | Part No. | Remark
--- | --- | ---
2‑inch HD viewfinder | AJ-HVF21KG | This is the viewfinder for Studio Handy Camera.
3.45-inch color viewfinder | AG-CVF10G AG-CVF15G | —
9‑inch LCD viewfinder | AK-HVF100G | This is the LCD viewfinder for Studio Handy Camera.
Lens | FUJINON/CANON | —
Camera Control Unit (CCU) | AK-UCU500P/AK-UCU500PS/AK-UCU500E/AK-UCU500ES | This is the camera control unit for Studio Handy Camera. It is connected to Studio Handy Camera using an optical fiber multi cable. Do not connect anything other than AK-UCU500P/AK-UCU500PS/AK-UCU500E/AK-UCU500ES.
Remote Operation Panel (ROP) | AK-HRP1000G AK-HRP1005G | This is connected to the CCU using the ROP cable to remotely control the camera, CCU, and lens.

Top of the page