- Top
- Menu Operations
- Menu list
- [NETWORK SETUP]

# [NETWORK SETUP]

[NETWORK SETUP] cannot be selected right after the power is turned on, because boot of the camera is in progress.

This is not an error. Perform operation after a while.

Item | Description of settings
--- | ---
[IP ADDRESS] | Sets the IP address. Factory setting: [192.168.0.30]
[SUBNET MASK] | Sets the subnet mask. Factory setting: [255.255.255.0]
[DEFAULT GATEWAY] | Sets the default gateway. Factory setting: [192.168.0.1]
[HTTP PORT] | Sets the port number of HTTP (port number when accessing with a browser). [1]…[65535] Factory setting: [80]
[ROP PORT] | Sets the port number when connecting to ROP. [49152], [49200]…[49299] Factory setting: [49152]
[SET EXCUTE] | Selects whether to execute with the configured settings. [NO], [YES]
[MAC ADDRESS] | Displays the MAC address. (This cannot be changed.)

Top of the page