- Top
- Menu Operations
- Menu list
- [MAINTENANCE]

# [MAINTENANCE]

## [CAC ADJUST]

[CAC ADJUST] cannot be selected right after the power is turned on, because boot of the camera is in progress.

This is not an error. Perform operation after a while.

Item | Description of settings
--- | ---
[CAC CONTROL] | Selects whether to perform maintenance of CAC files stored in the camera’s internal memory. [OFF], [ON] Factory setting: [ON]
[CAC FILE DELETE] | Selects a file to delete. [YES], [NO]
[CAC FILE NUMBER] | Selects a file. [1]…[32] Factory setting: [1]

## [LENS FILE ADJUST]

Item | Description of settings
--- | ---
[LENS FILE ADJUST] | [LENS FILE SW] | Switches the enable/disable of the lens file. [OFF], [ON] Factory setting: [OFF]
| [LENS FILE MODE] | Selects the operation mode. [LOAD], [STORE], [CANCEL] Factory setting: [LOAD]
| [FILE NO.] | Selects a file. When [LENS FILE MODE] is [LOAD]: [1]…[32] When [LENS FILE MODE] is [STORE]: [1]…[32] Factory setting: [1]
| [FILE NAME] | Enters a file name. (15 characters or less) Factory setting: [LENS FILE 1]
| [EXECUTE] | Selects whether to execute. [NO], [YES]
| [FLARE R] | Adjusts Rch flare of the data selected in [FILE NO.]. [−100]…[+100] Factory setting: [0]
| [FLARE G] | Adjusts Gch flare of the data selected in [FILE NO.]. [−100]…[+100] Factory setting: [0]
| [FLARE B] | Adjusts Bch flare of the data selected in [FILE NO.]. [−100]…[+100] Factory setting: [0]
| [GAIN R] | Adjusts Rch gain of the data selected in [FILE NO.]. [−100]…[+100] Factory setting: [0]
| [GAIN B] | Adjusts Bch gain of the data selected in [FILE NO.]. [−100]…[+100] Factory setting: [0]
| [W H SAW R] | Adjusts Rch white shading for the data selected in [FILE NO.] horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
| [W H SAW G] | Adjusts Gch white shading for the data selected in [FILE NO.] horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
| [W H SAW B] | Adjusts Bch white shading for the data selected in [FILE NO.] horizontally using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
| [W H PARA R] | Adjusts Rch white shading for the data selected in [FILE NO.] horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
| [W H PARA G] | Adjusts Gch white shading for the data selected in [FILE NO.] horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
| [W H PARA B] | Adjusts Bch white shading for the data selected in [FILE NO.] horizontally using a parabolic waveform. [−100]…[+100] Factory setting: [0]
| [W V SAW R] | Adjusts Rch white shading for the data selected in [FILE NO.] vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
| [W V SAW G] | Adjusts Gch white shading for the data selected in [FILE NO.] vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
| [W V SAW B] | Adjusts Bch white shading for the data selected in [FILE NO.] vertically using a saw-toothed waveform. [−100]…[+100] Factory setting: [0]
| [W V PARA R] | Adjusts Rch white shading for the data selected in [FILE NO.] vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]
| [W V PARA G] | Adjusts Gch white shading for the data selected in [FILE NO.] vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]
| [W V PARA B] | Adjusts Bch white shading for the data selected in [FILE NO.] vertically using a parabolic waveform. [−100]…[+100] Factory setting: [0]
| [EXTENDER1] | Sets the magnification of lens extender 1. [NONE], [0.1]…[9.9] Factory setting: [2.0]
| [EXTENDER2] | Sets the magnification of lens extender 2. [NONE], [0.1]…[9.9] Factory setting: [NONE]
| [EXTENDER3] | Sets the magnification of lens extender 3. [NONE], [0.1]…[9.9] Factory setting: [NONE]
| [EXTENDER4] | Sets the magnification of lens extender 4. [NONE], [0.1]…[9.9] Factory setting: [NONE]

## [F DROP ADJUST]

Item | Description of settings
--- | ---
[F DROP RANGE] | Sets the determination reference value for the F drop of the lens. [1]…[40] Factory setting: [10]

## [BLACK SHADING]

Item | Description of settings
--- | ---
[CORRECT] | Enables/disables the auto correction function of black shading. [OFF], [ON] Factory setting: [ON]
[DETECTION] | Selects whether to execute auto correction function of black shading. [NO], [YES]
[SAVE] | Selects whether to save the auto correction data. [NO], [YES]
[CLEAR] | Selects whether to clear the auto correction data. [NO], [YES]

## [FAN SETTING]

Item | Description of settings
--- | ---
[FAN] | [FAN MODE] | Sets the operation mode of the air cooling fan. [NORMAL], [SILENT], [POWERFUL], [OFF] Factory setting: [NORMAL]

## [B/U LIGHT ADJUST]

Item | Description of settings
--- | ---
[BOX SW(PUSH SW)] | Sets the luminance of the box switch of the Build-up Unit. [1]…[10] Factory setting: [5]
[LED(POWER)] | Sets the luminance of the lamp (<POWER>) of the Build-up Unit. [1]…[10] Factory setting: [5]
[LED(ND/CC)] | Sets the luminance of the lamp (<ND>/<CC>) of the Build-up Unit. [1]…[10] Factory setting: [5]
[CAM NO.(REAR)] | Sets the luminance of the rear side camera number of the Build-up Unit. [1]…[10] Factory setting: [5]
[CAM NO.(FRONT)] | Sets the luminance of the front side camera number of the Build-up Unit. [1]…[10] Factory setting: [5]

## [DATE/TIME]

[DATE/TIME] cannot be selected right after the power is turned on, because boot of the camera is in progress.

This is not an error. Perform operation after a while.

Item | Description of settings
--- | ---
[PRESENT] | Displays the present date and time.
[DATE YY] | Sets the year. [15]…[99] Factory setting: [16]
[DATE MM] | Sets the month. [01]…[12] Factory setting: [01]
[DATE DD] | Sets the day. [01]…[31] Factory setting: [01]
[TIME HH] | Sets the hour. [00]…[23] Factory setting: [00]
[TIME MM] | Sets the minute. [00]…[59] Factory setting: [00]
[SET EXECUTE] | Selects whether to save the configured details. [NO], [YES]
[RESET] | Selects whether to reset the settings. [NO], [YES]

## [INITIALIZE]

[READ FACTORY ALL DATA] cannot be selected right after the power is turned on, because boot of the camera is in progress.

This is not an error. Perform operation after a while.

Item | Description of settings
--- | ---
[MENU INITIALIZE] | Restores the value of [MAIN MENU] to their factory settings. [YES], [NO]
[READ USER ALL DATA] | Restores the values of [MAIN MENU], scene file and user file to their factory settings. [YES], [NO]
[READ FACTORY ALL DATA] | Restores the values of [MAIN MENU], scene file, user file, and the factory adjusted values to their factory settings. [YES], [NO]

## [UPDATE]

[UPDATE] cannot be selected right after the power is turned on, because boot of the camera is in progress.

This is not an error. Perform operation after a while.

Description of settings
Updates the software. Execute the update of the software with the update image file stored in the SD memory card. The busy lamp (next to the SD memory card slot) and the back tally lamp flash during the update of software is executing. [YES], [NO] Factory setting: [NO]

Top of the page