- Top
- Menu Operations
- Menu list
- [DISPLAY SETUP]

# [DISPLAY SETUP]

## [MARKER]

Item | Description of settings
--- | ---
[FOCUS ASSIST SW] | Enables/disables the focus assist switch. [OFF], [ON] Factory setting: [OFF]
[FOCUS ASSIST MODE] | — | Sets whether to cancel the focus assist by the switch or by the duration of time. [SW], [INSTANT] Factory setting: [SW]
| [CANCEL TIME] | Sets the duration of time before cancelling the focus assist when [INSTANT] is selected. [1sec], [3sec], [5sec], [10sec], [20sec] Factory setting: [5sec]
[FOCUS ASSIST] | — | Displays the type of the focus assist.
| [IN RED SW] | Enables/disables the IN RED switch. [OFF], [ON] Factory setting: [OFF]
| [IN RED COLOR] | Sets the color for IN RED. [RED], [GREEN], [BLUE], [WHITE] Factory setting: [RED]
| [SQUARE SW] | Enables/disables the SQUARE switch. [OFF], [ON] Factory setting: [OFF]
| [SQUARE COLOR] | Sets the color for the SQUARE. [RED], [GREEN] Factory setting: [GREEN]
| [BAR SW] | Enables/disables the BAR switch. [OFF], [ON] Factory setting: [OFF]
| [MAG SW] | Enables/disables the magnification display function. [OFF], [ON] Factory setting: [OFF]
[ZEBRA] | — | Enables/disables the luminance zebra. [OFF], [ON] Factory setting: [OFF]
| [ZEBRA1 LEVEL] | Sets the level of the luminance zebra 1. [0%]…[109%] Factory setting: [80%]
| [ZEBRA2 LEVEL] | Sets the level of the luminance zebra 2. [0%]…[109%] Factory setting: [100%]
| [ZEBRA PATTERN] | Sets the pattern of the luminance zebra. [1], [1+2], [SPOT] Factory setting: [1]
[FRAME LEVEL SWITCH] | — | Shows/hides the level display outside the frame marker. [OFF], [ON] Factory setting: [OFF]
| [FRAME LEVEL] | Sets the level to be displayed outside the frame marker. [0]…[31] Factory setting: [31]
[FRAME MARK SWITCH] | Shows/hides the frame marker. [OFF], [ON] Factory setting: [OFF]
[FRAME SIG] | Sets the aspect ratio of the frame marker. [4:3], [13:9], [14:9], [15:9], [16:9], [CINEMA], [VISTA] Factory setting: [4:3]
[SAFETY MARK1 SWITCH] | Shows/hides the safety marker 1. [OFF], [ON] Factory setting: [OFF]
[SAFETY MARK1] | Sets the aspect ratio of safety marker 1. [16:9], [15:9], [14:9], [13:9], [4:3] Factory setting: [16:9]
[SAFETY AREA1] | Sets the size of safety area 1. [80%]…[100%] Factory setting: [80%]
[SAFETY MARK2 SWITCH] | Shows/hides the safety marker 2. [OFF], [ON] Factory setting: [OFF]
[SAFETY MARK2] | Sets the aspect ratio of safety marker 2. [16:9], [15:9], [14:9], [13:9], [4:3] Factory setting: [4:3]
[SAFETY AREA2] | Sets the size of safety marker 2. [80%]…[100%] Factory setting: [93%]
[EFFECTIVE AREA MARK] | Shows/hides the effective area marker. [OFF], [ON] Factory setting: [OFF]
[PF LENS AREA MARK] | Shows/hides the auto focus area marker of the PF lens. [OFF], [AUTO] Factory setting: [OFF]
[CENTER MARK] | — | Shows/hides the center marker. [OFF], [ON] Factory setting: [OFF]
| [CENTER MARK SELECT] | Sets the size of the center marker. [1]…[8] Factory setting: [1]
| [LINE WIDTH] | Sets the thickness of the center marker frame. [1]…[3] Factory setting: [2]
[MARKER LEVEL] | Sets the brightness of the markers and on-screen display. [50%]…[100%] Factory setting: [100%]
[USER BOX] | — | Shows/hides the user box. [OFF], [ON] Factory setting: [OFF]
| [MEMORY SELECT] | Configures the memory of the user box. [1], [2], [3] Factory setting: [1]
| [H POSITION] | Adjusts the horizontal position of the user box. [−50]…[50] Factory setting: [0]
| [H OFFSET] | Finely adjusts the horizontal offset of the user box. [−10]…[10] Factory setting: [0]
| [V POSITION] | Adjusts the vertical position of the user box. [−50]…[50] Factory setting: [0]
| [V OFFSET] | Finely adjusts the vertical offset of the user box. [−10]…[10] Factory setting: [0]
| [WIDTH] | Adjusts the width of the user box. [0]…[100] Factory setting: [50]
| [HEIGHT] | Adjusts the height of the user box. [0]…[100] Factory setting: [50]
| [BOX/CROSS] | Sets the shape of the user box. [BOX], [CROSS] Factory setting: [BOX]
| [EFFECT MEMORY1] | Configures the valid memory of the user box. [OFF], [ON] Factory setting: [OFF]
| [EFFECT MEMORY2] | Configures the valid memory of the user box. [OFF], [ON] Factory setting: [OFF]
| [EFFECT MEMORY3] | Configures the valid memory of the user box. [OFF], [ON] Factory setting: [OFF]

## [VIEW FINDER DETAIL]

Item | Description of settings
--- | ---
[VIEW FINDER DETAIL] | Adjusts the details of the viewfinder. [0]…[23] Factory setting: [7]
[ZOOM LINK] | Enables/disables the details of the zoom-interlocked viewfinder. [OFF], [ON] Factory setting: [OFF]
[ZOOM LINK LEVEL] | Adjusts the detail level of the zoom-interlocked viewfinder. [1]…[5] Factory setting: [3]
[RETURN SIGNAL] | [HD PEAK FREQUENCY] | Adjusts the peak frequency of the return signal. [LOW], [MID], [HIGH] Factory setting: [LOW]
| [HD OFFSET GAIN] | Adjusts the detail offset gain of the return signal. [0]…[5] Factory setting: [0]
| [HD CRISP] | Adjusts the detail crisp level of the return signal. [0]…[63] Factory setting: [0]

## [VIEW FINDER DISPLAY]

Item | Description of settings
--- | ---
[F NUMBER] | Shows/hides the iris display (F value). [OFF], [ON] Factory setting: [OFF] This is displayed when you use a lens that outputs position information.
[ZOOM] | Shows/hides the zoom position display. [OFF], [ON] Factory setting: [OFF] This is displayed when you use a lens that outputs position information.
[FOCUS] | Shows/hides the focus position display. [OFF], [ON] Factory setting: [OFF] This is displayed when you use a lens that outputs position information.
[FOCUS CONDITION] | Shows/hides the focus information display. [OFF], [ON] Factory setting: [OFF]
[EXTENDER] | Shows/hides the extender display. [OFF], [ON] Factory setting: [OFF]
[FILTER] | Shows/hides the filter position display. [OFF], [ON] Factory setting: [OFF]
[MASTER GAIN] | Shows/hides the master gain display. [OFF], [ON] Factory setting: [OFF]
[OFFSET GAIN] | Shows/hides the offset gain display. [OFF], [ON] Factory setting: [OFF]
[SHUTTER] | Shows/hides the electronic shutter display. [OFF], [ON] Factory setting: [OFF]
[AUDIO LEVEL] | Shows/hides the audio level (level meter) display. [OFF], [ON] Factory setting: [OFF]
[DIGITAL EXTENDER] | Shows/hides the digital extender display. [OFF], [ON] Factory setting: [OFF]
[WHITE CHANNEL] | Shows/hides the white balance memory display. [OFF], [ON] Factory setting: [OFF]
[DRS] | Shows/hides the dynamic range stretcher display. [OFF], [ON] Factory setting: [OFF]
[CAC] | Shows/hides the chromatic aberration compensation (CAC) display. [OFF], [ON] Factory setting: [OFF]
[OPT LEVEL] | Shows/hides the display of the level of the optical signal received by the camera. [OFF], [ON] Factory setting: [OFF]
[RETURN SELECT] | Shows/hides the return ID display. [OFF], [ON] Factory setting: [OFF]
[STATUS] | Shows/hides the display appearing when functions are selected. [OFF], [ON] Factory setting: [OFF]
[STATUS(AUTO)] | Shows/hides the display appearing when AWB/ABB/ASU are activated or deactivated. [OFF], [ON] Factory setting: [OFF]
[SENSOR RATE] | Shows/hides the sensor imaging rate display. [OFF], [ON] Factory setting: [OFF]
[VOLTAGE] | Shows/hides the power supply display. [OFF], [ON] Factory setting: [OFF]
[SYSTEM MODE] | Shows/hides the system frequency/resolution display. [OFF], [ON] Factory setting: [OFF]
[FAN OFF] | Shows/hides the status display when the fan is off. [OFF], [ON] Factory setting: [OFF]
[MONI OUT SIGNAL] | Shows/hides the monitor output signal type display. [OFF], [ON] Factory setting: [OFF]
[COLOR TEMP] | Shows/hides the color temperature display. [OFF], [ON] Factory setting: [OFF]
[FBC] | Shows/hides the flash band compensation display. [OFF], [ON] Factory setting: [OFF]
[SHOOTING MODE] | Shows/hides the sensitivity mode display. [OFF], [ON] Factory setting: [OFF]
[LEVEL GAUGE] | Shows/hides the level gauge display. [OFF], [ON] Factory setting: [OFF]
[MAG] | Shows/hides the status display when the focus assist magnification display function is enabled. [OFF], [ON] Factory setting: [ON]
[MENU DISP WARNING] | Shows/hides the menu warning display. [OFF], [ON] Factory setting: [ON]
[F DROP ADJUST] | Shows/hides the F drop display. [OFF], [ON] Factory setting: [OFF]
[HDR] | Shows/hides the HDR display. [OFF], [ON] Factory setting: [OFF]
[CHARACTER SIZE] | Selects the character size for display on the viewfinder. [LARGE], [SMALL] Factory setting: [SMALL]
[DISPLAY TYPE] | Selects the black frame mode for display on the viewfinder. [NORMAL], [FRAME] Factory setting: [NORMAL]

## [MODE CHECK IND]

Item | Description of settings
--- | ---
[AUDIO] | Shows/hides the [AUDIO] screen during the mode check. [OFF], [ON] Factory setting: [ON]
[USER SW STATUS] | Shows/hides the [USER SW STATUS] screen during the mode check. [OFF], [ON] Factory setting: [ON]
[!LED] | Shows/hides the [!LED] screen during the mode check. [OFF], [ON] Factory setting: [ON]
[SDI OUT] | Shows/hides the [SDI OUT] screen during the mode check. [OFF], [ON] Factory setting: [ON]
[CAC] | Shows/hides the [CAC] screen during the mode check. [OFF], [ON] Factory setting: [ON]

## [!LED]

For items whose setting is [ON], the LED in the viewfinder () lights up when the operating status of the camera becomes irregular.

Item | Description of settings
--- | ---
[GAMMA OFF] | Shows/hides the status display when gamma is disabled. [OFF], [ON] Factory setting: [OFF]
[SHUTTER] | Shows/hides the status display when the electronic shutter is enabled. [OFF], [ON] Factory setting: [OFF]
[EXTENDER] | Shows/hides the status display when the lens extender is enabled. [OFF], [ON] Factory setting: [OFF]
[FAN OFF] | Shows/hides the status display when the fan is off. [OFF], [ON] Factory setting: [OFF]
[MASTER GAIN] | Shows/hides the status display when the gain is other than 0 dB. [OFF], [ON] Factory setting: [OFF]
[BLACK GAMMA] | Shows/hides the status display when the black gamma is enabled. [OFF], [ON] Factory setting: [OFF]
[!LED MODE] | Sets whether to use lighting of the LED () in the viewfinder as yellow tally function. [NORMAL], [YELLOW TALLY] Factory setting: [NORMAL]

Top of the page