- Top
- Menu Operations
- Menu list
- [HDR-PAINT]

# [HDR-PAINT]

Configures the image settings during HDR.

Item | Description of settings
--- | ---
[HLG MODE] | Sets the mode of HLG. [FIX]: Fixed mode [VAR]: Variable mode Factory setting: [FIX]
[SDR CONVERT MODE] | Selects the mode to convert to SDR. [FIX]: Fixed mode [VAR]: Variable mode Factory setting: [FIX]

## [GAMMA/BLACK GAMMA]

The setting will be disabled and cannot be set when [FIX] is selected for [HLG MODE].

Item | Description of settings
--- | ---
[BLACK GAMMA SW] | Enables/disables black gamma. [OFF], [ON] Factory setting: [OFF]
[MASTER BLACK GAMMA] | Adjusts the gamma characteristic adjacent to black. [−32]…[+32] Factory setting: [0]
[R BLACK GAMMA] | Adjusts the gamma characteristic of red adjacent to black to the master gamma. [−32]…[+32] Factory setting: [0]
[B BLACK GAMMA] | Adjusts the gamma characteristic of blue adjacent to black to the master gamma. [−32]…[+32] Factory setting: [0]

## [KNEE]

The setting will be disabled and cannot be set when [FIX] is selected for [HLG MODE].

Item | Description of settings
--- | ---
[KNEE SW] | — | Enables/disables knee. [OFF], [ON] Factory setting: [ON]
| [KNEE POINT] | Sets the knee point position. [60.00] - [100.00] (0.25 step) Factory setting: [80.00]
| [KNEE SLOPE] | Sets the knee slope. [00]…[199] Factory setting: [130]

## [SDR CONVERT]

The setting will be disabled and cannot be set when [FIX] is selected for [SDR CONVERT MODE].

Item | Description of settings
--- | ---
[GAIN] | Sets the gain of SDR. [−12], [−9], [−6], [−3], [0] Factory setting: [−6]
[CLIP] | Sets the clip of SDR. [LOW], [MID], [HIGH] Factory setting: [HIGH]

Top of the page