- Top
- Menu Operations
- Menu list
- [SWITCH MODE]

# [SWITCH MODE]

## [USER SWITCH]

Item | Description of settings
--- | ---
[GRIP RET] | Selects the grip <RET> switch function. [A], [B], [C], [PTT] Factory setting: [A]
[GRIP PTT] | Selects the grip <PTT> switch function. [PTT], [A], [B], [C] Factory setting: [PTT]
[LENS VTR] | Selects the <VTR> switch function of the handy lens. [A], [B], [C], [PTT], [D.EXT], [INH] Factory setting: [B]
[LENS RET1] | Selects the <RET1> switch function of the standard lens. [A], [B], [C], [PTT], [DISP], [MARK OFF], [LENS EXT], [D.EXT] , [C.TEMP], [CENTER], [ASSIST], [LVL G RESET] Factory setting: [A]
[LENS RET2] | Selects the <RET2> switch function of the standard lens. [A], [B], [C], [PTT], [DISP], [MARK OFF], [LENS EXT], [D.EXT] , [C.TEMP], [CENTER], [ASSIST], [LVL G RESET] Factory setting: [B]
[EXTERNAL RET1] | Selects the function of external return control switch 1. [A], [B], [C], [D.EXT] Factory setting: [A]
[EXTERNAL RET2] | Selects the function of external return control switch 2. [A], [B], [C], [D.EXT] Factory setting: [B]
[EXTERNAL RET3] | Selects the function of external return control switch 3. [A], [B], [C], [D.EXT] Factory setting: [B]
[USER SWITCH1] | Selects the function of the <USER 1> switch. [RETURN A], [RETURN B], [RETURN C], [PTT], [DISP], [MARK OFF], [D.EXT], [C.TEMP], [ASSIST], [CALL], [LVL G RESET] Factory setting: [RETURN A]
[USER SWITCH2] | Selects the function of the <USER 2> switch. [RETURN A], [RETURN B], [RETURN C], [PTT], [DISP], [MARK OFF], [D.EXT], [C.TEMP], [ASSIST], [CALL], [LVL G RESET] Factory setting: [PTT]
[USER SWITCH3] | Selects the function of the <USER 3> switch. [RETURN A], [RETURN B], [RETURN C], [PTT], [DISP], [MARK OFF], [D.EXT], [C.TEMP], [ASSIST], [CALL], [LVL G RESET] Factory setting: [PTT]
[USER SWITCH4] | Selects the function of the <USER 4> switch. [RETURN A], [RETURN B], [RETURN C], [PTT], [DISP], [MARK OFF], [D.EXT], [C.TEMP], [ASSIST], [CALL], [LVL G RESET] Factory setting: [PTT]
[USER B/U SWITCH1] | Selects the function of the user switch 1 on the Build-up Unit. [RETURN A], [RETURN B], [RETURN C], [PTT], [DISP], [MARK OFF], [LENS EXT], [D.EXT], [C.TEMP], [CENTER], [ASSIST], [LVL G RESET] Factory setting: [LENS EXT]
[USER B/U SWITCH2] | Selects the function of the user switch 2 on the Build-up Unit. [RETURN A], [RETURN B], [RETURN C], [PTT], [DISP], [MARK OFF], [LENS EXT], [D.EXT], [C.TEMP], [CENTER], [ASSIST], [LVL G RESET] Factory setting: [CENTER]
[USER B/U SWITCH3] | Selects the function of the user switch 3 on the Build-up Unit. [RETURN A], [RETURN B], [RETURN C], [PTT], [DISP], [MARK OFF], [LENS EXT], [D.EXT], [C.TEMP], [CENTER], [ASSIST], [LVL G RESET] Factory setting: [PTT]

## [GAIN SETTING]

Item | Description of settings
--- | ---
[LOW GAIN] | Sets the amount of gain increase when <L> is selected for the <GAIN> switch. [−6dB]…[36dB] When [MAIN MENU] → [SYSTEM MODE] → [SHOOTING MODE] → [NORMAL] is set: [−3dB]…[36dB] Factory setting: [0dB]
[OFFSET LOW GAIN] | Sets the offset from [LOW GAIN]. [−2.9dB]…[+2.9dB] (0.1 dB step) Factory setting: [0.0dB]
[MID GAIN] | Sets the amount of gain increase when <M> is selected for the <GAIN> switch. [−6dB]…[36dB] When [MAIN MENU] → [SYSTEM MODE] → [SHOOTING MODE] → [NORMAL] is set: [−3dB]…[36dB] Factory setting: [9dB]
[OFFSET MID GAIN] | Sets the offset from [MID GAIN]. [−2.9dB]…[+2.9dB] (0.1 dB step) Factory setting: [0.0dB]
[HIGH GAIN] | Sets the amount of gain increase when <H> is selected for the <GAIN> switch. [−6dB]…[36dB] When [MAIN MENU] → [SYSTEM MODE] → [SHOOTING MODE] → [NORMAL] is set: [−3dB]…[36dB] Factory setting: [18dB]
[OFFSET HIGH GAIN] | Sets the offset from [HIGH GAIN]. [−2.9dB]…[+2.9dB] (0.1 dB step) Factory setting: [0.0dB]

## [IRIS]

Item | Description of settings
--- | ---
[AUTO IRIS] | Enables/disables the auto iris mode. [OFF], [ON] Factory setting: [ON] (when the camera is used standalone), [OFF] (others)
[WINDOW SELECT] | Sets the photometric range. [1]…[4] The image of window will be as follows. [1] [2] [3] [4] Factory setting: [1]
[IRIS LEVEL] | Adjusts the target value (brightness) of the auto iris. [0]…[100] Factory setting: [50]
[PEAK RATIO] | Sets the ratio of the peak value and average value of auto iris photometry. [0]…[100] Factory setting: [50]
[IRIS RANGE] | Sets the fine adjustment range of the auto iris level using the iris adjustment joystick. [NORMAL], [(3/4)], [(2/4)], [(1/4)] Factory setting: [NORMAL]
[IRIS SPEED] | Sets the auto iris speed. [1]…[25] Factory setting: [15]
[IRIS GAIN] | Switches whether to adjust auto iris photometry speed adjustment with the iris gain volume of the lens or from the menu. Normally, set this to [LENS] and make adjustments with the iris volume of the lens. [LENS], [CAM] Factory setting: [LENS]
[LENS EXT COMP SW] | Sets the ALC compensation when the lens extender is enabled. [OFF], [ON] Factory setting: [OFF]
[EXTENDER1] | Sets the magnification of lens extender 1. [NONE], [0.1]…[9.9] Factory setting: [2.0]
[LENS EXT COMP LEVEL] | Sets the iris compensation level when lens extender 1 is enabled. [−100]…[+100] Factory setting: [0]
[EXTENDER2] | Sets the magnification of lens extender 2. [NONE], [0.1]…[9.9] Factory setting: [NONE]
[LENS EXT COMP LEVEL] | Sets the iris compensation level when lens extender 2 is enabled. [−100]…[+100] Factory setting: [0]
[EXTENDER3] | Sets the magnification of lens extender 3. [NONE], [0.1]…[9.9] Factory setting: [NONE]
[LENS EXT COMP LEVEL] | Sets the iris compensation level when lens extender 3 is enabled. [−100]…[+100] Factory setting: [0]
[EXTENDER4] | Sets the magnification of lens extender 4. [NONE], [0.1]…[9.9] Factory setting: [NONE]
[LENS EXT COMP LEVEL] | Sets the iris compensation level when lens extender 4 is enabled. [−100]…[+100] Factory setting: [0]

## [FBC SETTING]

Item | Description of settings
--- | ---
[FBC] | Enables/disables the flash band compensation. [OFF], [ON] Factory setting: [OFF]

## [W/B BAL SETTING]

Item | Description of settings
--- | ---
[W/B BAL SW] | Sets the conditions for activating the white balance switch. [NORMAL]: Enables the switch only when the camera is operated individually. [ALWAYS]: Always enables the switch. Factory setting: [NORMAL]
[ABB SW MODE] | Sets the switch of the black balance. [NORMAL], [PTT] Factory setting: [NORMAL]
[ABB SET MODE] | Sets the operation mode of the black balance. This cannot be set in HDR mode. [MODE1], [MODE2] Factory setting: [MODE1]
[AWB SET MODE] | Sets the operation mode of the automatic white balance. [MODE1], [MODE2] Factory setting: [MODE1]
[SHOCKLESS WB SW] | — | Enables/disables the shockless white balance when the color temperature is changed. [OFF], [ON] Factory setting: [OFF]
[SHOCKLESS WB SPEED] | Sets the speed of the shockless white balance. [1]…[5] Factory setting: [4]

## [SHUTTER SPEED]

Item | Description of settings
--- | ---
[SHUTTER SW] | Enables/disables the shutter function. [OFF]: Disables the shutter. [ON]: Enables the shutter speed with [SHUTTER SPEED]/[SYNCHRO SCAN]. Factory setting: [OFF]
[SHUTTER MODE] | Selects the operation mode of the shutter. [SHUTTER]: Sets the shutter speed to that configured for [SHUTTER SPEED]. [SYNCHRO]: Sets the shutter speed to that configured for [SYNCHRO SCAN]. Factory setting: [SHUTTER]
[SHUTTER SPEED] | Sets the shutter speed when [SHUTTER MODE] is [SHUTTER]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/100] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]
[SYNCHRO SCAN] | Sets the shutter speed when [SHUTTER MODE] is [SYNCHRO]. [59.94i]/[59.94p] mode: [61.7Hz]…[6130Hz] Factory setting: [61.7Hz] [50i]/[50p] mode: [51.5Hz]…[6250Hz] [29.97p] mode: [30.9Hz]…[2600Hz] [25p] mode: [25.7Hz]…[3130Hz] [23.98p] mode: [24.7Hz]…[2880Hz] [240fps] mode: [240Hz]…[6130Hz] Factory setting: [240Hz] [200fps] mode: [200Hz]…[6250Hz] Factory setting: [200Hz]

## [SHUTTER SELECT]

Item | Description of settings
--- | ---
[SHUTTER OFF BY ROP] | Selects whether to enable the shutter mode from ROP. [ENABLE], [DISABLE] Factory setting: [DISABLE]
[POSITION1] | Sets the shutter speed of [POSITION1]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/100] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/60] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/60] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/50] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/48] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]
[POSITION2] | Sets the shutter speed of [POSITION2]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/120] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/100] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/120] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/100] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/120] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]
[POSITION3] | Sets the shutter speed of [POSITION3]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/125] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/125] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/125] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/125] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/125] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]
[POSITION4] | Sets the shutter speed of [POSITION4]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]
[POSITION5] | Sets the shutter speed of [POSITION5]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/500] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/500] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/500] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/500] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/500] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]
[POSITION6] | Sets the shutter speed of [POSITION6]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1000] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1000] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1000] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1000] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1000] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]
[POSITION7] | Sets the shutter speed of [POSITION7]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1500] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1500] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1500] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1500] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/1500] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]
[POSITION8] | Sets the shutter speed of [POSITION8]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/2000] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/2000] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/2000] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/2000] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/2000] [200fps]/[240fps] mode: [1/250], [1/500], [1/1000], [1/1500], [1/2000] Factory setting: [1/250]

## [SHUTTER POSITION]

Item | Description of settings
--- | ---
[POSITION1] | Enables/disables the [POSITION1] settings of the shutter position. [OFF], [ON] Factory setting: [ON]
[POSITION2] | Enables/disables the [POSITION2] settings of the shutter position. [OFF], [ON] Factory setting: [ON]
[POSITION3] | Enables/disables the [POSITION3] settings of the shutter position. [OFF], [ON] Factory setting: [ON]
[POSITION4] | Enables/disables the [POSITION4] settings of the shutter position. [OFF], [ON] Factory setting: [ON]
[POSITION5] | Enables/disables the [POSITION5] settings of the shutter position. [OFF], [ON] Factory setting: [ON]
[POSITION6] | Enables/disables the [POSITION6] settings of the shutter position. [OFF], [ON] Factory setting: [ON]
[POSITION7] | Enables/disables the [POSITION7] settings of the shutter position. [OFF], [ON] Factory setting: [ON]
[POSITION8] | Enables/disables the [POSITION8] settings of the shutter position. [OFF], [ON] Factory setting: [ON]
[SHUTTER SELECT BY ROP] | Selects whether the shutter operation of ROP follows the [POSITION1] to [POSITION8] settings. [FULL], [SELECT] Factory setting: [SELECT]

Top of the page