- Top
- Menu Operations
- Menu operations
- Basic operations

# Basic operations

<MENU> button

Fig. 1

Jog dial button

Fig. 2

Fig. 3

Press the <MENU> button.

The [MAIN MENU] of the camera is displayed in the image output from the <HD SDI OUT 2> terminal. (Fig. 1)

Turn the jog dial button to select an item.

Press the jog dial button.

The menu of the selected item is accessed. (Fig. 2)

Turn the jog dial button to select an item.

Press the jog dial button.

The menu of the selected item is accessed. (Fig. 3)

Turn the jog dial button to select a menu item to configure.

Press the jog dial button.

The setting of the item indicated by the arrow flashes. (Fig. 3)

Turn the jog dial button to change the setting.

Press the jog dial button.

The setting is confirmed.

Pressing the <MENU> button to exit the menu screen also reflects the setting.

NOTE

- This can be changed quickly by pressing and turning the jog dial button.

## Entering characters

Fig. 1

Fig. 2

Fig. 3

Fig. 4

Press the jog dial button.

The cursor changes to arrow pointing down, and the cursor can be moved to next character (previous character) by turning the jog dial button. (Fig. 1, Fig. 2)

Turn the jog dial button to move the arrow over the character to be changed.

Press the jog dial button.

The character to be changed flashes. (Fig. 3)

Turn the jog dial button to change the character.

Press the jog dial button.

The setting is confirmed.

Perform the same operation for all characters to be changed.

Turn the jog dial button to move the arrow cursor to beginning of the menu items.

Press the jog dial button.

The cursor changes to a horizontal arrow and another item can be selected. (Fig. 4)

Top of the page