- Top
- Menu Operations
- Menu list
- [PAINT]

# [PAINT]

## [PAINT SWITCH]

Item | Description of settings
--- | ---
[WHITE SHADING] | Enables/disables the white shading (saw-toothed waveform or parabolic waveform). [OFF], [ON] Factory setting: [ON]
[FLARE] | Enables/disables flare. [OFF], [ON] Factory setting: [ON]
[GAMMA] | Enables/disables gamma. [OFF], [ON] Factory setting: [ON]
[BLACK GAMMA] | Enables/disables black gamma. [OFF], [ON] Factory setting: [OFF]
[KNEE] | Enables/disables knee. [OFF], [MANUAL], [AUTO] Factory setting: [MANUAL]
[WHITE CLIP] | Enables/disables white clips. [OFF], [ON] Factory setting: [ON]
[DRS SW] | Enables/disables dynamic range stretcher. [OFF], [ON] It is displayed as [---] in the UHD mode/UHD CROP mode. Factory setting: [OFF]
[DETAIL] | Enables/disables the detail. [OFF], [ON] Factory setting: [ON]
[SKIN TONE DETAIL] | Enables/disables the skin tone detail. [OFF], [ON] Factory setting: [OFF]
[MATRIX] | Enables/disables matrix (linear matrix/12-axis color correction). [OFF], [ON] Factory setting: [OFF]
[LINEAR MATRIX] | Enables/disables linear matrix. [OFF], [ON] Factory setting: [OFF]
[COLOR CORRECT] | Enables/disables 12-axis color correction. [OFF], [ON] Factory setting: [OFF]

## [PEDESTAL]

Item | Description of settings
--- | ---
[MASTER PEDESTAL] | Adjusts the black level of the master pedestal. [−99] - [99] Factory setting: [0]
[R PEDESTAL] | Sets the correction level of red to the master pedestal. [−800] - [+800] Factory setting: [0]
[G PEDESTAL] | Sets the correction level of green to the master pedestal. [−800] - [+800] Factory setting: [0]
[B PEDESTAL] | Sets the correction level of blue to the master pedestal. [−800] - [+800] Factory setting: [0]
[PEDESTAL OFFSET] | Sets whether to maintain the Rch, Gch, and Bch pedestal levels after adjusting the automatic black balance. [ON]: Maintains the values set in [R PEDESTAL], [G PEDESTAL], and [B PEDESTAL]. [OFF]: Sets [R PEDESTAL], [G PEDESTAL], and [B PEDESTAL] to [0]. Factory setting: [OFF]

## [CHROMA]

Item | Description of settings
--- | ---
[CHROMA LEVEL SWITCH] | Enables/disables the gain adjustment of chroma. [OFF], [ON] Factory setting: [OFF]
[CHROMA LEVEL] | Sets the gain adjustment of chroma. [−100%] - [+40%] Factory setting: [0%]

## [COLOR TEMP SETTING]

Item | Description of settings
--- | ---
[COLOR TEMP PRESET] | [COLOR TEMP PRE SWITCH] | Enables/disables the color temperature adjustment. [OFF], [ON] Factory setting: [OFF]
| [COLOR TEMP] | Sets the color temperature when [COLOR TEMP PRE SWITCH] is [ON]. [2000K] - [15000K] Factory setting: [3200K]
| [R GAIN] | Sets the correction level of red to the color temperature. [−400] - [+400] Factory setting: [0]
| [B GAIN] | Sets the correction level of blue to the color temperature. [−400] - [+400] Factory setting: [0]
| [G AXIS] | Sets the correction level of green to the color temperature. [−400] - [+400] Factory setting: [0]
[COLOR TEMP] | [COLOR TEMP] | Sets the color temperature when the white balance is executed. [2000K] - [15000K] Factory setting: [3200K]
| [R GAIN] | Sets the correction level of red to the color temperature. [−400] - [+400] Factory setting: [0]
| [B GAIN] | Sets the correction level of blue to the color temperature. [−400] - [+400] Factory setting: [0]
| [G AXIS] | Sets the correction level of green to the color temperature. [−400] - [+400] Factory setting: [0]

## [RB GAIN CONTROL SETTING]

Item | Description of settings
--- | ---
[RB GAIN PRESET] | [R GAIN] | Sets the preset value of Rch gain. This is not available when [COLOR TEMP PRE SWITCH] is set to [OFF]. [−1000] - [+1000] Factory setting: [0]
| [B GAIN] | Sets the preset value of Bch gain. This is not available when [COLOR TEMP PRE SWITCH] is set to [OFF]. [−1000] - [+1000] Factory setting: [0]
[RB GAIN] | [R GAIN] | Sets the correction level of red to the gain. [−1000] - [+1000] Factory setting: [0]
| [B GAIN] | Sets the correction level of blue to the gain. [−1000] - [+1000] Factory setting: [0]
| [GAIN OFFSET] | Sets if the gain levels of Rch and Bch are maintained when the automatic white balance is adjusted. [ON]: Maintains the values set with [R GAIN] and [B GAIN]. [OFF]: The values for [R GAIN] and [B GAIN] is set to [0]. Factory setting: [OFF]

## [WHITE SHADING]

Item | Description of settings
--- | ---
[CORRECT] | Enables/disables the white shading (saw-toothed waveform or parabolic waveform) correction. [OFF], [ON] Factory setting: [ON]
[H SAW R] | Adjusts the white shading gain for Rch horizontally using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[H SAW G] | Adjusts the white shading gain for Gch horizontally using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[H SAW B] | Adjusts the white shading gain for Bch horizontally using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[H PARA R] | Adjusts the white shading gain for Rch horizontally using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[H PARA G] | Adjusts the white shading gain for Gch horizontally using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[H PARA B] | Adjusts the white shading gain for Bch horizontally using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[V SAW R] | Adjusts the white shading gain for Rch vertically using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[V SAW G] | Adjusts the white shading gain for Gch vertically using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[V SAW B] | Adjusts the white shading gain for Bch vertically using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[V PARA R] | Adjusts the white shading gain for Rch vertically using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[V PARA G] | Adjusts the white shading gain for Gch vertically using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[V PARA B] | Adjusts the white shading gain for Bch vertically using a parabolic waveform. [−100] - [+100] Factory setting: [0]

## [FLARE]

Item | Description of settings
--- | ---
[FLARE] | Enables/disables flare correction. [OFF], [ON] Factory setting: [ON]
[MASTER FLARE] | Adjusts the master flare. [−100] - [+100] Factory setting: [0]
[R FLARE] | Adjusts the Rch flare. [−100] - [+100] Factory setting: [0]
[G FLARE] | Adjusts the Gch flare. [−100] - [+100] Factory setting: [0]
[B FLARE] | Adjusts the Bch flare. [−100] - [+100] Factory setting: [0]

## [GAMMA/BLACK GAMMA]

Item | Description of settings
--- | ---
[GAMMA] | Enables/disables gamma correction. [OFF], [ON] Factory setting: [ON]
[GAMMA MODE SELECT] | Selects the type of gamma. [HD], [FILMLIKE1], [FILMLIKE2], [FILMLIKE3], [FILM REC], [VIDEO REC] Factory setting: [HD]
[MASTER GAMMA] | Adjusts the gamma characteristic. When [GAMMA MODE SELECT] is [HD]: [0.150] - [0.750] (0.0020 step) When [GAMMA MODE SELECT] is [FILMLIKE1]/[FILMLIKE2]/[FILMLIKE3]: [0.3000] - [0.7500] (0.0025 step) When [GAMMA MODE SELECT] is [FILE REC]/[VIDEO REC]: [0.150] - [0.750] (0.0020 step) When [MAIN MENU] → [PAINT] → [DRS] → [DRS] is [ON]: [0.150] - [0.750] (0.0020 step) Factory setting: [0.450]
[R GAMMA] | Adjusts the gamma characteristic of red to the master gamma. [−75] - [+75] Factory setting: [0]
[B GAMMA] | Adjusts the gamma characteristic of blue to the master gamma. [−75] - [+75] Factory setting: [0]
[BLACK STRECH LEVEL] | (Only when [FILM REC] is set) Sets the position of the gamma stretch. [0%] - [30%] Factory setting: [0%]
[DYNAMIC LEVEL] | (Only when [FILM REC] is set) Sets dynamic range. [200%], [300%], [400%], [500%] Factory setting: [500%]
[KNEE POINT] | (Only when [VIDEO REC] is set) Sets the knee point. [30] - [90] Factory setting: [30]
[KNEE SLOPE] | (Only when [VIDEO REC] is set) Sets the knee slope. [150%]/[200%]/[250%]/[300%]/[350%]/[400%]/[450%]/[500%]/[550%]/[600%] Factory setting: [150%]
[BLACK GAMMA] | Enables/disables black gamma. This cannot be set when [MAIN MENU] → [PAINT] → [DRS] → [DRS] → [ON] is set. [OFF], [ON] Factory setting: [OFF]
[MASTER BLACK GAMMA] | Adjusts the gamma characteristic adjacent to black. [−32] - [+32] Factory setting: [0]
[R BLACK GAMMA] | Adjusts the gamma characteristic of red adjacent to black to the master gamma. [−20] - [+20] Factory setting: [0]
[B BLACK GAMMA] | Adjusts the gamma characteristic of blue adjacent to black to the master gamma. [−20] - [+20] Factory setting: [0]

## [KNEE]

The setting becomes disabled and cannot be set in the following cases.

- When [GAMMA/BLACK GAMMA] → [GAMMA MODE SELECT] is set to [FILE REC]/[VIDEO REC]

- When [MAIN MENU] → [PAINT] → [DRS] → [DRS] is set to [ON]

Item | Description of settings
--- | ---
[KNEE] | — | Enables/disables the knee function. [OFF], [MANUAL], [AUTO] Factory setting: [MANUAL]
| [KNEE MASTER POINT] | Sets the knee point position. [080.00%] - [110.00%] (0.25% step) Factory setting: [95.00%]
| [KNEE R POINT] | Adjusts the knee point of red to [KNEE MASTER POINT]. [−25.00%] - [25.00%] (0.25% steps) Factory setting: [0.00%]
| [KNEE B POINT] | Adjusts the knee point of blue to [KNEE MASTER POINT]. [−25.00%] - [25.00%] (0.25% steps) Factory setting: [0.00%]
| [KNEE MASTER SLOPE] | Sets the knee slope. [00] - [199] Factory setting: [130]
| [KNEE R SLOPE] | Adjusts the knee slope of red to [KNEE MASTER SLOPE]. [−99] - [+99] Factory setting: [0]
| [KNEE B SLOPE] | Adjusts the knee slope of blue to [KNEE MASTER SLOPE]. [−99] - [+99] Factory setting: [0]
| [AUTO KNEE POINT] | Sets the break position of the auto knee. [080.00%] - [107.00%] Factory setting: [95%]
| [AUTO KNEE LEVEL] | Sets the maximum level of the auto knee. [100%] - [109%] Factory setting: [108%]
| [AUTO KNEE RESPONSE] | Sets the response speed of the auto knee. The smaller the setting value, the faster the response speed. [1] - [8] Factory setting: [4]

## [WHITE CLIP]

Item | Description of settings
--- | ---
[WHITE CLIP] | Enables/disables the white clip function. [OFF], [ON] Factory setting: [ON]
[MASTER WHITE CLIP LEVEL] | Sets the white clip level. [80%] - [109%] Factory setting: [109%]
[R WHITE CLIP LEVEL] | Adjusts red to [MASTER WHITE CLIP LEVEL]. [−15%] - [+15%] Factory setting: [0%]
[B WHITE CLIP LEVEL] | Adjusts blue to [MASTER WHITE CLIP LEVEL]. [−15%] - [+15%] Factory setting: [0%]
[HI-COLOR] | Sets whether to improve the color reproduction in high-luminance areas. [OFF], [ON] Factory setting: [OFF]
[HI-COLOR LEVEL] | Sets the level of the mode that expands the color dynamic range. [1] - [32] Factory setting: [32]

## [DRS]

Item | Description of settings
--- | ---
[DRS] | Enables/disables the dynamic range stretcher function. Set this to [ON] to automatically adjust the contrast. [OFF], [ON] It is displayed as [---] in the UHD mode/UHD CROP mode. Factory setting: [OFF]
[EFFECT DEPTH] | Sets the compression level of the high-luminance areas of the dynamic range stretcher function. Set a larger value to increase the compression level of the high-luminance areas. [1] - [5] It is displayed as [---] in the UHD mode/UHD CROP mode. Factory setting: [5]

## [DETAIL SETTING]

Item | Description of settings
--- | ---
[DETAIL] | Enables/disables all detail functions. [OFF], [ON] Factory setting: [ON]
[MASTER DETAIL] | Sets the master detail. [−31] - [+31] Factory setting: [0]
[H DETAIL LEVEL] | Sets the correction level of the horizontal detail. [00] - [63] Factory setting: [20] (UHD mode/UHD CROP mode), [15] (HD mode)
[V DETAIL LEVEL] | Sets the correction level of the vertical detail. [00] - [63] Factory setting: [32] (UHD mode/UHD CROP mode), [27] (HD mode)
[PEAK FREQUENCY] | Sets the peak frequency of the horizontal detail. UHD mode/UHD CROP mode: [0] - [4] HD mode: [00] - [31] Factory setting: [3] (UHD mode/UHD CROP mode), [18] (HD mode)
[V DETAIL FREQUENCY] | Sets the vertical detail frequency. UHD mode/UHD CROP mode: [0] - [4] HD mode: [00] - [31] Factory setting: [3] (UHD mode/UHD CROP mode), [18] (HD mode)
[CRISP] | Sets the detail signal noise removal level. [00] - [63] Factory setting: [5] (UHD mode/UHD CROP mode), [0] (HD mode)
[DETAIL GAIN(+)] | Sets the detail level in the + (upward) direction. It is displayed as [---] in the UHD mode/UHD CROP mode. [−31] - [+31] Factory setting: [0]
[DETAIL GAIN(−)] | Sets the detail level in the − (downward) direction. It is displayed as [---] in the UHD mode/UHD CROP mode. [−31] - [+31] Factory setting: [0]
[DETAIL CLIP+] | Adjust the detail clip to reduce glare produced by an excess of details. [00] - [63] Factory setting: [0]
[DETAIL CLIP−] | Adjusts the length of the undershoot of the detail edge component. [00] - [63] Factory setting: [0]
[DETAIL SOURCE] | Sets the RGB signal component ratio to create the detail. [(G+R)/2], [(G+B)/2], [(2G+B+R)/4], [(3G+R)/4], [R], [G] It is displayed as [---] in the UHD mode/UHD CROP mode. Factory setting: [(G+R)/2]
[KNEE APERTURE LEVEL] | Adjusts the knee aperture level. [00] - [39] Factory setting: [0] (UHD mode/UHD CROP mode), [5] (HD mode)
[LEVEL DEPENDENT SWITCH] | Enables/disables the function to remove details of dark areas. [OFF], [ON] Factory setting: [ON] (UHD mode/UHD CROP mode), [OFF] (HD mode)
[LEVEL DEPENDENT] | Sets the level to remove details of dark areas. [00] - [15] Factory setting: [8]

## [DOWNCON DETAIL SETTING]

This item is not displayed in the HD mode.

Item | Description of settings
--- | ---
[DETAIL] | Enables/disables all detail functions. [OFF], [ON] Factory setting: [ON]
[MASTER DETAIL] | Sets the master detail. [−31] - [+31] Factory setting: [0]
[H DETAIL LEVEL] | Sets the correction level of the horizontal detail. [00] - [63] Factory setting: [15]
[V DETAIL LEVEL] | Sets the correction level of the vertical detail. [00] - [63] Factory setting: [15]
[PEAK FREQUENCY] | Sets the peak frequency of the horizontal detail. [00] - [31] Factory setting: [10]
[V DETAIL FREQUENCY] | Sets the vertical detail frequency. [00] - [31] Factory setting: [10]
[CRISP] | Sets the detail signal noise elimination level. [00] - [63] Factory setting: [10]
[DETAIL GAIN(+)] | Sets the detail level in the + (upward) direction. [−31] - [+31] Factory setting: [0]
[DETAIL GAIN(−)] | Sets the detail level in the − (downward) direction. [−31] - [+31] Factory setting: [0]
[DETAIL CLIP+] | Adjust the detail clip to reduce glare produced by an excess of details. [00] - [63] Factory setting: [0]
[DETAIL CLIP−] | Adjusts the length of the undershoot of the detail edge component. [00] - [63] Factory setting: [0]
[DETAIL SOURCE] | Sets the RGB signal component ratio to create the detail. [(G+R)/2], [(G+B)/2], [(2G+B+R)/4], [(3G+R)/4], [R], [G] Factory setting: [(G+R)/2]
[KNEE APERTURE LEVEL] | Adjusts the knee aperture level. [00] - [39] Factory setting: [00]
[LEVEL DEPENDENT SWITCH] | Enables/disables the function to eliminate the detail in the dark areas. [OFF], [ON] Factory setting: [OFF]
[LEVEL DEPENDENT] | Sets the level to eliminate the detail in the dark areas. [00] - [15] Factory setting: [8]

## [SKIN TONE DETAIL SETTING]

Item | Description of settings
--- | ---
[SKIN TONE DETAIL] | Enables/disables the skin tone detail function. [OFF], [ON] Factory setting: [OFF]
[SKIN GET] | — | Selects whether to automatically obtain the color saturation and hue information from the cursor position. [NO], [YES]
| [MEMORY SELECT] | Selects the skin tone table of the subject to apply the skin tone table to. [A], [B], [C] Factory setting: [A]
| [CURSOR] | Shows/hides the box cursor in the center of the screen. [OFF], [ON] Factory setting: [OFF]
| [H POSITION] | Adjusts the horizontal position of the cursor. [0%] - [100.00%] (0.25% steps) Factory setting: [50.00%]
| [V POSITION] | Adjusts the vertical position of the cursor. [0%] - [100.00%] (0.25% steps) Factory setting: [50.00%]
[ZEBRA] | — | Enables/disables the zebra display. [OFF], [ON] Factory setting: [OFF]
| [ZEBRA EFFECT MEMORY] | Selects the table of the zebra display. [A], [B], [C], [A+B], [A+C], [B+C], [A+B+C] Factory setting: [A+B+C]
[SKIN TONE EFFECT MEMORY] | Selects the skin tone table used to apply the skin tone detail. [A], [B], [C], [A+B], [A+C], [B+C], [A+B+C] Factory setting: [A+B+C]
[SKIN TONE CRISP] | Adjusts the skin tone detail. [−63] - [+63] Factory setting: [+63]
[I CENTER] | Sets the center position on the I axis (the area where the skin tone effect is applied). [0] - [255] Factory setting: [87] (UHD mode/UHD CROP mode), [18] (HD mode)
[I WIDTH] | Sets the width of the area where the skin tone effect is applied on the I axis with [I CENTER] being the center. [0] - [255] Factory setting: [20] (UHD mode/UHD CROP mode), [8] (HD mode)
[Q WIDTH] | Sets the width of the area where the skin tone effect is applied on the Q axis with [I CENTER] being the center. [0] - [255] Factory setting: [43]
[Q PHASE] | Sets the phase of the area where the skin tone effect is applied with the Q axis being the reference. [0] - [359] Factory setting: [90]

## [LINEAR MATRIX]

Item | Description of settings
--- | ---
[MATRIX] | Enables/disables the matrix function. [OFF], [ON] Factory setting: [OFF]
[LINEAR MATRIX] | — | Enables/disables the linear matrix function. [OFF], [ON] Factory setting: [OFF]
| [LINEAR TABLE] | Selects the table for linear matrix. [A], [B] Factory setting: [A]
[COLOR CORRECT] | — | Enables/disables the 12-axis color correction function. [OFF], [ON] Factory setting: [OFF]
| [COLOR CORRECT TABLE] | Selects the table for color correction. [A], [B] Factory setting: [A]
[MATRIX (R-G)_N] | Adjusts the linear matrix between red and green. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (R-G)_P] | Adjusts the linear matrix between red and green. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (R-B)_N] | Adjusts the linear matrix between red and blue. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (R-B)_P] | Adjusts the linear matrix between red and blue. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (G-R)_N] | Adjusts the linear matrix between green and red. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (G-R)_P] | Adjusts the linear matrix between green and red. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (G-B)_N] | Adjusts the linear matrix between green and blue. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (G-B)_P] | Adjusts the linear matrix between green and blue. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (B-R)_N] | Adjusts the linear matrix between blue and red. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (B-R)_P] | Adjusts the linear matrix between blue and red. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (B-G)_N] | Adjusts the linear matrix between blue and green. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]
[MATRIX (B-G)_P] | Adjusts the linear matrix between blue and green. This item is not available when [MATRIX] is set to [OFF]. [−31] - [+31] Factory setting: [0]

## [COLOR CORRECTION]

Item | Description of settings
--- | ---
[MATRIX] | Enables/disables the matrix function. [OFF], [ON] Factory setting: [OFF]
[LINEAR MATRIX] | — | Enables/disables the linear matrix function. [OFF], [ON] Factory setting: [OFF]
| [LINEAR TABLE] | Selects the table for linear matrix. [A], [B] Factory setting: [A]
[COLOR CORRECT] | — | Enables/disables the 12-axis color correction function. [OFF], [ON] Factory setting: [OFF]
| [COLOR CORRECT TABLE] | Selects the table for color correction. [A], [B] Factory setting: [A]
[G SAT] | Adjusts green color saturation. [−127] - [+126] Factory setting: [0]
[CY-G SAT] | Adjusts the color saturation between green and cyan. [−127] - [+126] Factory setting: [0]
[CY SAT] | Adjusts cyan color saturation. [−127] - [+126] Factory setting: [0]
[B-CY SAT] | Adjusts the color saturation between cyan and blue. [−127] - [+126] Factory setting: [0]
[B SAT] | Adjusts blue color saturation. [−127] - [+126] Factory setting: [0]
[MG-B SAT] | Adjusts the color saturation between blue and magenta. [−127] - [+126] Factory setting: [0]
[MG_SAT] | Adjusts magenta color saturation. [−127] - [+126] Factory setting: [0]
[R-MG SAT] | Adjusts the color saturation between magenta and red. [−127] - [+126] Factory setting: [0]
[R SAT] | Adjusts red color saturation. [−127] - [+126] Factory setting: [0]
[YL-R SAT] | Adjusts the color saturation between red and yellow. [−127] - [+126] Factory setting: [0]
[YL SAT] | Adjusts yellow color saturation. [−127] - [+126] Factory setting: [0]
[G-YL SAT] | Adjusts the color saturation between yellow and green. [−127] - [+126] Factory setting: [0]
[G PHASE] | Adjusts green hue. [−127] - [+127] Factory setting: [0]
[CY-G PHASE] | Adjusts the hue between green and cyan. [−127] - [+127] Factory setting: [0]
[CY PHASE] | Adjusts cyan hue. [−127] - [+127] Factory setting: [0]
[B-CY PHASE] | Adjusts the hue between cyan and blue. [−127] - [+127] Factory setting: [0]
[B PHASE] | Adjusts blue hue. [−127] - [+127] Factory setting: [0]
[MG-B PHASE] | Adjusts the hue between blue and magenta. [−127] - [+127] Factory setting: [0]
[MG_PHASE] | Adjusts magenta hue. [−127] - [+127] Factory setting: [0]
[R-MG PHASE] | Adjusts the hue between magenta and red. [−127] - [+127] Factory setting: [0]
[R PHASE] | Adjusts red hue. [−127] - [+127] Factory setting: [0]
[YL-R PHASE] | Adjusts the hue between red and yellow. [−127] - [+127] Factory setting: [0]
[YL PHASE] | Adjusts yellow hue. [−127] - [+127] Factory setting: [0]
[G-YL PHASE] | Adjusts the hue between yellow and green. [−127] - [+127] Factory setting: [0]

## [SKIN CORRECTION]

Item | Description of settings
--- | ---
[SKIN AREA SW] | Enables/disables the function to finely adjust the color of the skin tone area. [OFF], [ON] Factory setting: [OFF]
[SKIN AREA TABLE] | Selects the table for the skin tone area. [A], [B] Factory setting: [A]
[SKIN AREA HUE] | Finely adjusts the hue of the skin tone area. [−127] - [+127] Factory setting: [0]
[SKIN AREA TONE] | Finely adjusts the tone of the skin tone area. [−127] - [+126] Factory setting: [0]

## [DNR]

Item | Description of settings
--- | ---
[DNR SW] | Enables/disables the noise reduction function. [OFF], [ON] Factory setting: [ON]
[DNR LEVEL] | Sets the level for the noise reduction. The larger the value, the stronger the noise reduction effect. [1] - [5] Factory setting: [3]

## [HAZE REDUCTION]

Item | Description of settings
--- | ---
[HAZE REDUCTION] | Enables/disables the haze elimination function. [OFF], [ON] Factory setting: [OFF]
[HAZE REDUCTION LEVEL] | Sets the level of the haze elimination. The larger the value, the stronger the haze elimination effect. [1] - [3] Factory setting: [1]

## [SCENE FILE]

Item | Description of settings
--- | ---
[MODE] | Selects the operation mode. [LOAD], [STORE] Factory setting: [LOAD]
[FILE NO.] | Selects a file number. When [MODE] is [LOAD]: [OFF], [1] - [8] When [MODE] is [STORE]: [1] - [8] Factory setting: [OFF]
[FILE NAME] | Enters a file name. (15 characters or less) Factory setting: [SCENE1]
[EXECUTE] | Selects whether to execute with the configured settings. [NO], [YES]

Top of the page