- Top
- Connecting to External Devices
- Connecting the remote operation panel (AK-HRP200G)
- IP connection with the <LAN> terminal

# IP connection with the <LAN> terminal

AK-HRP200G

<LAN> terminal

Connect the <LAN> terminal of this camera to the <LAN> terminal of the remote operation panel AK-HRP200G.

- Use the LAN cross cable when connecting without going through a hub.

- Use the LAN straight cable when connecting going through a hub.

#### Functions that can be controlled

The same functions as the serial connection can be used.

Top of the page