- Top
- Operation
- Convenient shooting functions
- Focus assist function

# Focus assist function

The focus assist function enables you to focus the target easily.

Expanded display, focus assist color display (display where the contour of the image is bordered with the selected color), and focus bar can be displayed in the output from the <HD SDI OUT 2> terminal.

## Focus assist color display

Set to [MAIN MENU] → [DISPLAY SETUP] → [MARKER] → [FOCUS ASSIST] → [IN RED SW] → [ON] in advance.

Select either of [RED]/[GREEN] in [MAIN MENU] → [DISPLAY SETUP] → [MARKER] → [FOCUS ASSIST] → [IN RED COLOR].

The contour of the image is bordered with the selected color when set to [MAIN MENU] → [DISPLAY SETUP] → [MARKER] → [FOCUS ASSIST] → [IN RED SW] → [ON]. At this time, the screen frame will be in the selected color.

Adjust the focus so that the contour of the subject to focus will turn into the selected color.

NOTE

- Displayed only in the output from the <HD SDI OUT 2> terminal.

## Focus bar display

The focus bar is displayed when set to [MAIN MENU] → [DISPLAY SETUP] → [MARKER] → [FOCUS ASSIST] → [BAR SW] → [ON].

The degree of focus is indicated by the length of the bar.

Not in focus

The bar extends to the right when the viewfinder is in-focus.

- White bar: Focus bar display

- Green line: Peak display

Top of the page