- Top
- Operation
- Convenient shooting functions
- Scan reverse shooting

# Scan reverse shooting

Image can be displayed reversed vertically or horizontally by setting [MAIN MENU] → [SYSTEM MODE] → [SCAN REVERSE].

NOTE

- The scan reverse in vertical direction will not operate for the output image from the <LAN> terminal in following cases.

  - [MAIN MENU] → [SYSTEM MODE] → [FORMAT] → [2160/60p], and [MAIN MENU] → [IN/OUT SELECT] → [SDI1 OUT FMT] → [720/60p]

  - [MAIN MENU] → [SYSTEM MODE] → [FORMAT] → [2160/59.94p], and [MAIN MENU] → [IN/OUT SELECT] → [SDI1 OUT FMT] → [720/59.94p]

  - [MAIN MENU] → [SYSTEM MODE] → [FORMAT] → [2160/50p], and [MAIN MENU] → [IN/OUT SELECT] → [SDI1 OUT FMT] → [720/50p]

Top of the page