- Top
- Menu Operations
- Menu list
- [SWITCH MODE]

# [SWITCH MODE]

## [ND FILTER]

Item | Description of settings
--- | ---
[ND FILTER] | Selects the ND filter. [CLEAR], [1/4], [1/16], [1/64] Factory setting: [CLEAR]

## [DIGITAL EXTENDER]

Item | Description of settings
--- | ---
[DIGITAL EXTENDER] | Enables/disables the function to double the image by digital process. [OFF], [ON] Factory setting: [OFF]

## [GAIN SETTING]

Item | Description of settings
--- | ---
[GAIN SELECT] | Switches the gain switch. [LOW], [MID], [HIGH], [S.GAIN1], [S.GAIN2], [S.GAIN3] Factory setting: [LOW]
[LOW GAIN] | Sets the gain increase volume when [LOW] is selected in [GAIN SELECT]. [−6dB] - [36dB] (3 dB steps) Factory setting: [0dB]
[MID GAIN] | Sets the gain increase volume when [MID] is selected in [GAIN SELECT]. [−6dB] - [36dB] (3 dB steps) Factory setting: [9dB]
[HIGH GAIN] | Sets the gain increase volume when [HIGH] is selected in [GAIN SELECT]. [−6dB] - [36dB] (3 dB steps) Factory setting: [18dB]

## [SUPER GAIN]

Item | Description of settings
--- | ---
[MEMORY SELECT] | Selects the save table for the super gain. [S.GAIN1], [S.GAIN2], [S.GAIN3] Factory setting: [S.GAIN1]
[TOTAL GAIN] | Displays the total of [GAIN] and [FRAME MIX].
[GAIN] | Sets the gain increase volume. [0dB] - [36dB] (3 dB steps) Factory setting: [30dB] ([S.GAIN1]), [36dB] ([S.GAIN2]), [36dB] ([S.GAIN3])
[FRAME MIX] | Sets the gain increase volume by accumulation. [OFF], [+6dB] - [+24dB] (6 dB steps) Factory setting: [OFF] ([S.GAIN1]), [+12dB] ([S.GAIN2]), [+24dB] ([S.GAIN3])
[H DETAIL LEVEL] | Sets the level of the horizontal detail. [0] - [63] Factory setting: [20] (UHD mode), [15] (HD mode)
[CRISP] | Sets the detail signal noise removal level. [0] - [63] Factory setting: [5] (UHD mode), [0] (HD mode)
[LEVEL DEPENDENT SWITCH] | Enables/disables the function to eliminate the detail in the dark areas. [OFF], [ON] Factory setting: [ON]
[LEVEL DEPENDENT] | Eliminates the detail in the dark areas. The larger the value, the range to eliminate is larger. [0] - [15] Factory setting: [8]
[PEAK FREQUENCY] | Sets the peak frequency of the horizontal detail. UHD mode: [0] - [4] HD mode: [0] - [31] Factory setting: [3] (UHD mode), [18] (HD mode)
[MASTER GAMMA] | Adjusts the gamma characteristic. When [MAIN MENU] → [PAINT] → [GAMMA/BLACK GAMMA] → [GAMMA MODE SELECT] is set to [HD]: [0.150] - [0.750] (0.0020 steps) When [MAIN MENU] → [PAINT] → [GAMMA/BLACK GAMMA] → [GAMMA MODE SELECT] is set to [FILMLIKE1]/[FILMLIKE2]/[FILMLIKE3]: [0.300] - [0.750] (0.0025 steps) When [MAIN MENU] → [PAINT] → [GAMMA/BLACK GAMMA] → [GAMMA MODE SELECT] is set to [FILE REC]/[VIDEO REC]: [0.150] - [0.750] (0.0020 steps) When [MAIN MENU] → [PAINT] → [DRS] → [DRS] is set to [ON]: [0.150] - [0.750] (0.0020 steps) Factory setting: [0.50] ([S.GAIN1]), [0.60] ([S.GAIN2]), [0.60] ([S.GAIN3])
[MASTER PEDESTAL OFFSET] | Adjusts the black level. [−200] - [+200] Factory setting: [000]
[R PEDESTAL OFFSET] | Adjusts the compensation value of the pedestal of Rch. [−200] - [+200] Factory setting: [000]
[B PEDESTAL OFFSET] | Adjusts the compensation value of the pedestal of Bch. [−200] - [+200] Factory setting: [000]

## [IRIS]

Item | Description of settings
--- | ---
[WINDOW SELECT] | Sets the photometric range. [1] - [4] The image of window will be as follows. [1] [2] [3] [4] Factory setting: [1]
[IRIS LEVEL] | Adjusts the target value (brightness) of the auto iris. [0] - [100] Factory setting: [50]
[PEAK RATIO] | Sets the ratio of the peak value and average value of auto iris photometry. [0] - [100] Factory setting: [50]
[IRIS RANGE] | Sets the fine adjustment range of the auto iris level by ROP. [NORMAL], [(3/4)], [(2/4)], [(1/4)] Factory setting: [NORMAL]
[IRIS SPEED] | Sets the auto iris speed. [1] - [25] Factory setting: [15]
[IRIS GAIN] | Switches whether to adjust auto iris photometry speed adjustment with the iris gain volume of the lens or from the menu. Normally, set this to [LENS] and make adjustment with the iris gain volume of the lens. [LENS], [CAM] Factory setting: [LENS]
[LENS EXT COMP SW] | Sets the iris compensation when the lens extender is enabled. [OFF], [ON] Factory setting: [OFF]
[LENS EXT COMP LEVEL] | Sets the iris compensation value when the lens extender is enabled. [−100] - [+100] Factory setting: [0]
[IRIS OFFSET SW] | Enables/disables the compensation against the iris control value. [OFF], [ON] Factory setting: [OFF]
[IRIS OFFSET] | Compensates the iris control value from the camera. [−100] - [+100] Factory setting: [0]

## [FBC SETTING]

It is displayed as [---] in the UHD mode/UHD CROP mode.

Item | Description of settings
--- | ---
[FBC] | Enables/disables the flash band compensation. [OFF], [ON] Factory setting: [OFF]

## [W/B BAL SETTING]

Item | Description of settings
--- | ---
[AWB SET] | Executes the automatic white balance. [NO], [YES]
[ABB SET] | Executes the automatic black balance. [NO], [YES]

## [SHUTTER SPEED]

Item | Description of settings
--- | ---
[SHUTTER SW] | Enables/disables the shutter function. [OFF]: Disables the shutter. [ON]: Enables the shutter speed with [SHUTTER SPEED]/[SYNCHRO SCAN]. Factory setting: [OFF]
[SHUTTER MODE] | Selects the operation mode of the shutter. [SHUTTER]: Sets the shutter speed to that configured for [SHUTTER SPEED]. [SYNCHRO]: Sets the shutter speed to that configured for [SYNCHRO SCAN]. Factory setting: [SHUTTER]
[SHUTTER SPEED] | Sets the shutter speed when [SHUTTER MODE] is [SHUTTER]. [59.94i]/[59.94p] mode: [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] [50i]/[50p] mode: [1/60], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] [29.97p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] [25p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] [23.98p] mode: [1/48], [1/50], [1/60], [1/96], [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/100]
[SYNCHRO SCAN DISP] | Sets the unit to display the synchro scan mode. [SEC]: Displays in time. [DEG]: Displays at shutter open angle. Factory setting: [SEC]
[SYNCHRO SCAN] | Sets the shutter speed when [SHUTTER MODE] is [SYNCHRO]. [59.94i]/[59.94p] mode: [61.7Hz] - [6130Hz] Factory setting: [61.7Hz] [50i]/[50p] mode: [51.5Hz] - [6250Hz] Factory setting: [51.5Hz] [29.97p] mode: [30.9Hz] - [2600Hz] Factory setting: [30.9Hz] [25p] mode: [25.7Hz] - [3130Hz] Factory setting: [25.7Hz] [23.98p] mode: [24.7Hz] - [2880Hz] Factory setting: [24.7Hz] When [DEG] is displayed: [3.0deg] - [359.5deg] Factory setting: [180.0deg]

## [TALLY]

Item | Description of settings
--- | ---
[FRONT TALLY] | Sets enable/disable and brightness of the front tally lamp. [OFF], [LOW], [HIGH] Factory setting: [LOW]
[BACK TALLY] | Sets enable/disable and brightness of the back tally lamp. [OFF], [LOW], [HIGH] Factory setting: [LOW]

## [BAR SETTING]

Item | Description of settings
--- | ---
[BAR SW] | Enables/disables the color bar. [OFF], [ON] Factory setting: [OFF]
[BAR SELECT] | Sets the type of the color bar. [FULL], [SMPTE], [ARIB] Factory setting: [FULL]

Top of the page