- Top
- Menu Operations
- Menu list
- [INTELLIGENT]

# [INTELLIGENT]

## [INTELLIGENT MEMORY]

Item | Description of settings
--- | ---
[MEMORY] | Switches the target memory for the intelligent function. [1], [2] Factory setting: [1]
[MASTER GAIN] | Displays the current total of gain.
[ND FILTER] | Displays the current position of the ND filter.
[INTELLIGENT] | Sets the operation mode of the intelligent function. [OFF]: Operates with the setting from the menu or the camera controller. [ON]: Performs the automatic exposure and auto tracking white balance. [LOCK]: Maintains the automatic exposure and auto tracking white balance adjustment status of the point when [ON] is switched to [LOCK]. Factory setting: [OFF]
[INTELLIGENT MODE] | Sets the control item of the intelligent function. [AE]: Controls the gain (including [FRAME MIX]) and the automatic exposure by changing the ND filter when it cannot be adjusted within the range of [IRIS RANGE]. [ATW]: Adjusts the white balance automatically when it is determined that there is white subject. [AE+ATW]: Performs [AE] and [ATW] simultaneously. Factory setting: [AE+ATW]
[ND FILTER SELECT] | Sets the ND filter that is in operation for automatic exposure. Control from the camera control cannot be performed during operation for automatic exposure. [CLEAR], [1/4], [1/16], [1/64], [AUTO] Factory setting: [AUTO]
[AGC SPEED] | Sets the convergence time for the auto gain control. The larger the value, the faster the convergence time. [1] - [5] Factory setting: [3]
[AGC GAIN STEP] | Sets the steps for gain increase or gain decrease for the auto gain control. [NORMAL]: Gain is increased in fine steps from 0 dB to the value set in [AGC MAX GAIN] when underexposed. Gain is decreased in fine steps from the value set in [AGC MAX GAIN] to 0 dB when overexposed. [MAX]: Gain is increased in coarse steps from 0 dB to the value set in [AGC MAX GAIN] when underexposed. Gain is decreased in coarse steps from the value set in [AGC MAX GAIN] to 0 dB when overexposed. Set [AGC MAX GAIN] so it will not exceed the movable range of the lens iris when set to [MAX]. Factory setting: [NORMAL]
[HIGH LIGHT DETECT] | Sets the level of ignorance in 10 steps when a spot light enters the valid image. The larger the value, the more it will response to spot light. [1] - [10] Factory setting: [5]
[IRIS LIMIT] | Sets the iris control range for the auto gain control operation. [1]: F2.0 - F8 [2]: F2.0 - F11 [3]: F2.0 - F16 Factory setting: [2]
[ATW SPEED] | Sets the convergence time for the auto tracking white balance in 5 steps. The larger the value, the faster the convergence time. [1] - [5] Factory setting: [3]
[ATW WIDTH] | Sets the range of color temperature to follow with the auto tracking white balance. [1] - [5] Factory setting: [5]
[D5600K] | Sets if the center value of the auto tracking white balance is to be set to 5600 K. [OFF], [ON] Factory setting: [ON]
[AGC MODE] | Sets the control mode for the auto gain control. [NORMAL]: Increases the gain up to +18 dB by the control of the auto gain control. [SPORTS]: Controls in accordance with an image with fast movement. [SN]: Controls by prioritizing SN. Factory setting: [NORMAL]
[AGC MAX GAIN] | Displays the maximum gain increase of the auto gain control.
[FRAME MIX] | Displays the amount of maximum frame addition by the auto gain control.

## [INTELLIGENT SETTING]

Item | Description of settings
--- | ---
[INTELLIGENT] | Switches the intelligent mode. [OFF]: Both [INTELLIGENT1] and [INTELLIGENT2] will be manual. [INTEL1]: [INTELLIGENT1] will be auto and [INTELLIGENT2] will be manual. [INTEL2]: [INTELLIGENT1] will be manual and [INTELLIGENT2] will be auto. Factory setting: [OFF]
[IRIS ON LOCK] | Selects the operating condition of the iris when the intelligent function is locked. [LOCK]: Maintains the iris in the lock start condition. [MANUAL]: Switches to manual operation. [PANEL]: Switches the auto/manual of the iris operation by the control from the camera controller. Factory setting: [LOCK]

Top of the page