- Top
- Operation
- Adjustment for shooting
- Shutter mode/speed setting

# Shutter mode/speed setting

It is possible to limit the range of shutter speed selection or to use the synchro scan mode in advance with [MAIN MENU] → [SWITCH MODE] → [SHUTTER SPEED] → [SHUTTER SPEED]/[SHUTTER MODE].

The selected shutter speed will be maintained even after the power of the unit is turned off.

NOTE

- Whichever mode the electronic shutter is used in, the higher the shutter speed, the lower the sensitivity of the camera becomes.

- When the aperture is in the automatic mode, it will increasingly open and the depth of focus will become shallower as the shutter speed is increased.

- Under lighting conditions using fluorescent lighting or other discharge tube, horizontal stripes might appear on screen. If this happens, this can be improved by adjusting the shutter speed.

- A subject that quickly crosses the camera may appear distorted when shot. This is due to the method applied for reading the signals from the pickup device (MOS sensor), and is not a malfunction.

- The shutter mode is turned off when the intelligent function is operating.

## Shutter related screen display

For details, refer to “On-screen displays of the monitor”.

Top of the page