- Top
- Connecting to External Devices
- Connecting the remote camera controller (AW-RP50N/AW-RP50E/AW-RP120G)

# Connecting the remote camera controller (AW-RP50N/AW-RP50E/AW-RP120G)

- Some of the functions can be controlled remotely by connecting the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G (optional).

- The unit can be controlled without using the pan/tilt head by the direct connection control of the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G.

NOTE

- Update the version of the remote camera controller as described below.

  AW-RP50N/AW-RP50E: 3.30.00 or later

  AW-RP120G: 2.40.00 or later

- For details, refer to the operating instructions of the remote camera controller and supplied flyer.

Serial connection with the <I/F> terminal
IP connection with the <LAN> terminal
Top of the page