- Top
- Maintenance
- Warning displays
- Camera warning displays

# Camera warning displays

#### When AWB (automatic white balance) is executed

[AWB HIGH LIGHT NG] | Automatic white balance cannot be executed because the light amount is excessive. Set the light amount to an appropriate level.
[AWB LOW LIGHT NG] | Automatic white balance cannot be executed because the light amount is insufficient. Set the light amount to an appropriate level.
[AWB RCH OUT RANGE] | The white balance convergence for red cannot be achieved. Shoot a uniformly white object on the screen, and execute AWB.
[AWB BCH OUT RANGE] | The white balance convergence for blue cannot be achieved. Shoot a uniformly white object on the screen, and execute AWB.

#### When ABB (automatic black balance) is executed

[ABB RCH OUT RANGE] | The black balance convergence for red cannot be achieved. Check if there are any errors in the image.
[ABB BCH OUT RANGE] | The black balance convergence for blue cannot be achieved. Check if there are any errors in the image.
[ABB GCH OUT RANGE] | The black balance convergence for green cannot be achieved. Check if there are any errors in the image.
[ABB NG] | The lens iris may not be closed.

#### Executing black shading

[BSHD NG] | An error has occurred with the black shading. Check if the lens is correctly closed.

Top of the page