- Top
- Web Screen
- [Setup] screen
- [Multi-screen setup] screen

# [Multi-screen setup] screen

[Multi-screen setup] screen sets the camera to display in the multi-screen.

Item | Description of settings
--- | ---
[IP address] | Enter the IP address of the camera to display in the multi-screen. Maximum of four groups with four cameras in each group (16 cameras) can be registered. Enter as follows when the HTTP port number of the camera to display is changed. (Example) 192.168.0.40:8080 Factory setting: [selfcamera] ([Cam1]), no registration ([Cam2] to [Cam16]) NOTE [IP address] is set with this unit for the camera displaying [selfcamera] as the IP address.
[Camera title] | Enter the title of the camera. Entered title of the camera is displayed in the multi-screen screen. You can enter 0 to 20 single-byte characters. Factory setting: parts No. display ([Cam1]), blank ([Cam2] to [Cam16]) Characters that can be used Single-byte numbers: 0123456789 Single-byte alphabet (upper/lower case): ABCDEFGHIJKLMNOPQRSTUVWXYZ abcdefghijklmnopqrstuvwxyz Single-byte symbols: !#$%'()*+,-./:;<=>?@[]^_`{|}~\ NOTE Only part of the camera title may display when 16 screen multi-screen is selected. Display of the multi-screen will be 4:3.

Top of the page