- Top
- Operation
- Multi-formats
- Superimposing of character

# Superimposing of character

Characters to be superimposed to output of each terminal are as follows.

- ✓: Superimposed.

- —: Not superimposed.

Output terminal | Character to superimpose
--- | ---
Camera ID | Menu and status
<UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals | — | —
<HD SDI OUT 1> terminal | ✓*1 | ✓*1
<HD SDI OUT 2> terminal | ✓ | ✓
<LAN> terminal | ✓*2 | ✓*2

Character is superimposed when [MAIN MENU] → [IN/OUT SELECT] → [HD-SDI1 CHAR] → [ON] is set.

Character is superimposed when [MAIN MENU] → [IN/OUT SELECT] → [LAN CHAR] → [ON] is set.

NOTE

- The method to display the menu when [MAIN MENU] → [IN/OUT SELECT] → [HD-SDI1 CHAR] is set to [OFF] is as follows.

  - Connect a monitor to the <HD SDI OUT 2> terminal.

  - Connect a PC to the <LAN> terminal, and use the UB300 Setting Tool.

Top of the page