- Top
- UB300 Setting Tool
- Connection

# Connection

Connect the personal computer to operate the UB300 Setting Tool and AK-UB300G as follows.

LAN cable (cross cable: optional)

When hub is used

Hub

LAN cable (straight cable: optional)

Set the IP address of the personal computer with a separate address of AK-UB300G within the range of private address.

Set the subnet mask to the same address as AK-UB300G.

(Example)

- Personal computer: 192.168.0.100

- AK-UB300G: 192.168.0.40

Top of the page