- Top
- Overview
- Using the camera in a system
- Expanded configuration devices

# Expanded configuration devices

In addition to the basic configuration devices, following devices can be connected.

Part name | Part No. | Remark
--- | --- | ---
Indoor pan/tilt head | AW-PH400P/AW-PH400E | —
Protocol converter | AW-IF400G | This is the converter to control the indoor pan/tilt head from the remote camera controller.
12G output board | AK-UHD12G | The 12G SDI signal or the 3G SDI signal can be output by installing to the camera.

Top of the page