- Top
- Web Screen
- Displaying the web screen
- Notes on the web screen

# Notes on the web screen

## IP address and subnet mask

Set the IP address of your computer to a different one from that of the camera within the private address range, and set the subnet mask address to the same as that of the camera.

IP address and subnet mask of the camera (factory settings)

- IP address: 192.168.0.40

- Subnet mask: 255.255.255.0

- Private address range: 192.168.0.0 to 192.168.0.255

## Computer environment required to display the web screen

For details on the computer environment required to display the web screen, refer to “Required environment for computer”.

Some of the functions on the [Setup] screen are only available on computers operating on Windows. Such functions are not available for computers operating on OS X (Mac).

Functions that are only available for Windows are indicated with (Windows).

To display the IP images of the camera on a computer running Windows, the plugin software for display, Network Camera View 4S, must be installed. This is not necessary with computers operating on OS X (Mac). (Installing the plugin software for display)

Top of the page