- Top
- Specifications
- Details of the connector signals

# Details of the connector signals

DC IN
| 1 | UNREG GND
2 | Not used
3 | Not used
4 | +12 V
HA16RA-4P(77) (Hirose Electric Co.) NOTE Use the external power supply with correct polarity.

TALLY OUT
| 1 | GND
2 | R TALLY (open collector)
3 | G TALLY (open collector)
4 | UNREG+12 V (max. 0.5 A)
HR10A-7R-4SC (73) (Hirose Electric Co.)

IRIS
| 1 | Return control
2 | REC-START/STOP
3 | GND
4 | Iris manual switching
5 | Iris control
6 | UNREG +12 V (max. 0.75 A)
7 | IRIS-POSI
8 | IRIS-G-MAX
9 | EXT-POSI
10 | Zoom position information
11 | LENS-RXD
12 | LENS-TXD
HR10A-10R-12SC (71) (Hirose Electric Co.)

ZOOM/FOCUS
| 1 | Focus control switching
2 | Zoom control switching
3 | GND
4 | Not used
5 | Not used
6 | Not used
7 | Not used
8 | Focus control
9 | Zoom control
10 | Not used
11 | COM+V voltage
12 | COM−V voltage
HR10A-10R-12PC(71) (Hirose Electric Co.)

I/F
| 1 | GND
2 | Not used
3 | Not used
4 | TX_N (EIA422)/TXD (EIA232) output
5 | RX_N (EIA422)/RXD (EIA232) input
6 | Not used
7 | G/L signal input
8 | Not used
9 | TX_P (EIA422) output
10 | RX_P (EIA422) input
11 | GND
12 | Not used
13 | GND
14 | GND
15 | GND
D02-M15SAG-20L9E (Japan Aviation Electronics Industry)

#### I/F cable specification

Use a cable equivalent or higher performance than the following description.

- Connect with AW-RP50N/AW-RP50E/AW-RP120G/AK-HRP200G

  AK-UB300G

  <I/F> terminal side

  AW-RP50N/AW-RP50E/AW-RP120G

  <TO PAN/TILT HEAD> terminal side

  GND

  AK-HRP200G

  Not used

  <RS-422> terminal side

  Not used

  GND

  TX_N (EIA422)/TXD (EIA232) output

  Not used

  RX_N (EIA422)/RXD (EIA232) input

  TX_N

  Not used

  RX_N

  G/L signal input

  RX_P

  TX_P

  Not used

  Not used

  TX_P (EIA422) output

  Not used

  RX_P (EIA422) input

  Use twisted-pair cable

  GND

  Use twisted-pair cable

  Not used

  GND

  GND

  GND

- Connecting with AK-HRP1000G/AK-HRP1005G

  AK-UB300G

  <I/F> terminal side

  GND

  AK-HRP1000G/AK-HRP1005G

  <CCU> terminal side

  Not used

  Not used

  CAM_DATA (H)

  CAM_DATA (L)

  TX_N (EIA422)/TXD (EIA232) output

  CAM_CONT (H)

  RX_N (EIA422)/RXD (EIA232) input

  Not used

  CAM_CONT (L)

  G/L signal input

  CAM No.A

  CAM No.B

  Not used

  CAM No.C

  TX_P (EIA422) output

  CAM No.D

  RX_P (EIA422) input

  +12 V

  GND

  Not used

  GND

  GND

  Use twisted-pair cable

  Use twisted-pair cable

  GND

  GND

NOTE

- For the connector of the connecting destination of the I/F cable, refer to the operating instruction of the corresponding device.

Top of the page