- Top
- Connecting to External Devices
- Connecting the indoor pan/tilt head (AW-PH400P/AW-PH400E)

# Connecting the indoor pan/tilt head (AW-PH400P/AW-PH400E)

- Some of the functions of this camera mounted on the indoor pan/tilt head can be remotely controlled by connecting the indoor pan/tilt head AW-PH400P/AW-PH400E (optional), protocol converter AW-IF400G (optional), and remote camera controller AW-RP50N/AW-RP50E/AW-RP120G (optional).

NOTE

- For the version of the remote camera controller, contact your dealer.

- For details, refer to the operating instructions of the indoor pan/tilt head, the protocol converter, and the remote camera controller, and supplied flyer.

Connecting with the <I/F> terminal
Top of the page