- Top
- Connecting to External Devices
- Connecting the remote operation panel (AK-HRP1000G/AK-HRP1005G)
- IP connection with the <LAN> terminal

# IP connection with the <LAN> terminal

AK-HRP1000G

AK-HRP1005G

<LAN> terminal

Connect the <LAN> terminal of this camera to the <LAN> terminal of the remote operation panel AK-HRP1000G/AK-HRP1005G.

- Use the LAN cross cable when connecting without going through a hub.

- Use the LAN straight cable when connecting going through a hub.

Set the [CONNECT SETTING] menu to [LAN(AW)] with the remote operation panel AK-HRP1000G/AK-HRP1005G.

#### Functions that can be controlled

The same functions as the serial connection can be used.

NOTE

- Supply the power of the remote operation panel AK-HRP1000G/AK-HRP1005G from the <LAN> terminal.

- Use an Ethernet hub and the PoE injector when supplying PoE power from the <LAN> terminal.

- For the Ethernet hub and the PoE injector that the operation have been confirmed, contact your dealer.

Top of the page