- Top
- Connecting to External Devices
- Connecting the remote camera controller (AW-RP50N/AW-RP50E/AW-RP120G)
- IP connection with the <LAN> terminal

# IP connection with the <LAN> terminal

(Example 1) When connecting without going through a hub

or

AW-RP120G

AW-RP50N/AW-RP50E

<LAN> terminal

(Example 2) When connecting going through a hub

AW-RP120G

Hub

<LAN> terminal

AW-RP50N/AW-RP50E

Connect the <LAN> terminal of this unit to the <LAN> terminal of the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G.

- Use the LAN cross cable when connecting without going through a hub.

- Use the LAN straight cable when connecting going through a hub.

Set the remote camera controller to IP direct connection control (IP_Direct).

#### Functions that can be controlled

The same functions as the serial connection can be used.

Top of the page