- Top
- Operation
- Image quality adjustment
- Chroma setting function

# Chroma setting function

This function sets color saturation and phase. It applies effects on whole images. It cannot be set to individual color hue.

#### General settings

[CHROMA LEVEL]: Sets the chroma level for the PR signal and the PB signal.

When the vector scope is used, the distance from the center (no color) increases or decreases in the whole image.

#### Advanced settings

No setting items are provided.

Top of the page