- Top
- Overview
- Using the camera in a system
- System block diagram

# System block diagram

## One-to-one configuration

This is the configuration to connect one AK-UB300G and one remote camera controller or the remote operation panel.

(AK-UB300G)

1. Remote control lens

2. HD monitor (for HD main line)

3. HD monitor (for HD monitor)

4. External DC power supply

5. UHD/HD monitor (for UHD/HD main line)

6. AW-RP120G

7. AW-RP50N/AW-RP50E

8. AK-HRP200G

9. AK-HRP1000G

10. AK-HRP1005G

- Video output

  For UHD mode

  - For UHD main line: Use the output from the <UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals.

  - For HD main line: Use the output from the <HD SDI OUT 1> terminal.

  - For HD monitor: Use the output from the <HD SDI OUT 2> terminal.

  For UHD CROP mode/HD mode

  - For HD main line: Use the output from the <HD SDI OUT 1> terminal, or the output from the <UHD/HD SDI OUT 1>/<UHD/HD SDI OUT 2> terminal.

  - For HD monitor: Use the output from the <HD SDI OUT 2> terminal.

  NOTE

- Pressing the <MENU> button will display the menu in the output from the <HD SDI OUT 2> terminal.

- Remote camera controller

  Connect AW-RP50N/AW-RP50E or AW-RP120G to the <I/F> terminal or the <LAN> terminal.

- Remote operation panel

  Connect AK-HRP200G, AK-HRP1000G, or AK-HRP1005G to the <I/F> terminal or the <LAN> terminal.

## Configuration using the indoor pan/tilt head

This is the configuration to connect one AK-UB300G, indoor pan/tilt head, and one remote camera controller.

#### AW-PH400P/AW-PH400E

(AK-UB300G)

1. Remote control lens

2. AW-PH400P/AW-PH400E

3. Relay cable

   Use the relay cable when connecting the zoom/focus control cable of the remote control lens to AW-PH400P/AW-PH400E. The device may be damaged when connected directly.

4. AW-CA15H29G

5. HD monitor (for HD main line)

6. External DC power supply

7. UHD/HD monitor (for UHD/HD main line)

8. HD monitor (for HD main line/monitor)

9. AW-IF400G

10. AW-RP120G

11. AW-RP50N/AW-RP50E

- Video output

  For UHD mode

  - For UHD main line: Use the output from the <UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals.

  - For HD main line: Use the output from the <HD SDI OUT 1> terminal.

  - For HD main line/monitor: Use the output from the <SDI> terminal of AW-PH400P/AW-PH400E.

  For UHD CROP mode/HD mode

  - For HD main line: Use the output from the <HD SDI OUT 1> terminal, or the output from the <UHD/HD SDI OUT 1>/<UHD/HD SDI OUT 2> terminal.

  - For HD main line/monitor: Use the output from the <SDI> terminal of AW-PH400P/AW-PH400E.

  NOTE

- Pressing the <MENU> button will display the menu in the output from the <HD SDI OUT 2> terminal.

- Remote camera controller

  Connect AW-RP50N/AW-RP50E or AW-RP120G to the <IP/RP> terminal of AW-PH400P/AW-PH400E.

#### Relay cable specification

Do not connect the pin number 6.

HR10A-10P-12S(73)

(Hirose Electric Co.)

HR10A-10J-12P(73)

(Hirose Electric Co.)

Top of the page