- Top
- Connecting to External Devices
- Connecting the indoor pan/tilt head (AW-PH400P/AW-PH400E)
- Connecting with the <I/F> terminal

# Connecting with the <I/F> terminal

AW-CA15H29G

<I/F> terminal

AW-IF400G

LAN straight cable

AW-PH400P/AW-PH400E

LAN straight cable

AW-RP120G

AW-RP50N/AW-RP50E

Connect the <I/F> terminal of this camera to the <CAMERA I/F> terminal of the indoor pan/tilt head AW-PH400P/AW-PH400E.

Connect the <PAN-TILT HEAD> terminal of the protocol converter AW-IF400G to the <IP/RP> terminal of the indoor pan/tilt head AW-PH400P/AW-PH400E.

Connect the <TO PAN/TILT HEAD> terminal of the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G to the <CONTROLLER> terminal of the protocol converter AW-IF400G.

Select [4] in [MAIN MENU] → [IN/OUT SELECT] → [PROTCOL] → [PROTCOL].

Select [Serial] in the connection setting of the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G.

In the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G, press and hold the <CAMERA STATUS/SELECTION> or <CAMERA SELECT/GROUP SELECT> button where this camera is assigned.

The camera model number is displayed at the top, and the [POWER] at the bottom of the LCD panel.

In the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G, select [ON] by turning the <F2> dial while holding down the <CAMERA STATUS/SELECTION> or <CAMERA SELECT/GROUP SELECT> button, and press the <F2> dial.

For the functions that will operate, refer to the AW-RP50N/AW-RP50E/AW-RP120G supported function list in following website.

http://pro-av.panasonic.net/

However, the UHD crop function cannot be controlled.

NOTE

- Use AW-CA15H29G (optional) for the cable to connect this camera to the indoor pan/tilt head.

- Perform one of the following operations to operate the auto iris of this camera using the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G.

  - Connect the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G directly to the camera, and set the IRIS setting to AUTO using the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G.

  - Connect the remote operation panel AK-HRP200G/AK-HRP1000G/AK-HRP1005G directly to the camera, and set the IRIS setting to AUTO using the remote operation panel AK-HRP200G/AK-HRP1000G/AK-HRP1005G.

  - Connect a PC to the camera, start up UB300 Setting Tool, and set the IRIS setting to AUTO using UB300 Setting Tool.

- Set the IRIS setting of the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G to AUTO once to establish the operation of the IRIS when the protocol converter AW-IF400G and the indoor pan/tilt head AW-PH400P/AW-PH400E are started after the IRIS setting is changed.

- Set IRIS setting to AUTO in the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G when using the intelligent function.

- Set the switch at the rear of the protocol converter AW-IF400G as follows.

  <SW1>switch: <OFF>

  <SW2>switch: <OFF>

  <SET UP> switch

  - <1>: <ON>

  - <2>: <OFF>

  - <3>: <ON> (300°) or <OFF> (190°)

  - <4>: <OFF>

Top of the page