- Top
- Overview
- Frame frequency setting

# Frame frequency setting

When the camera is shipped, the frame frequency is not set. Before using the camera for the first time, follow the steps below to set the frame frequency.

Fig. 1

Fig. 2

Connect a monitor to the <HD SDI OUT 2> terminal (<HD SDI OUT 2> terminal).

Connect the DC power supply.

The [SELECT FORMAT TYPE] screen is displayed.

Turn the jog dial button to move the cursor (arrow) to the frequency to set. (Fig. 1)

Press the jog dial button.

The confirmation screen is displayed.

Move the cursor (arrow) to [YES] and press the jog dial button. (Fig. 2)

The menu screen is displayed, and the setting is completed.

This screen is not displayed again when the power is turned on next and subsequently once this is set.

Disconnect the DC power supply.

Turn on the DC power supply.

Top of the page