- Top
- Web Screen
- [Live] screen (multi display mode)
- [Multi-screen] button

# [Multi-screen] button

Selects the display method of the [Live] screen.

1. [Single]

   Displays the IP image of the connected camera.

2. [4Split 1/4 Group], [4Split 2/4 Group], [4Split 3/4 Group], [4Split 4/4 Group], [16Split]

   Multiple IP images can be displayed in a single screen by setting the cameras to display in multi-screen with multi-screen setting screen [Multi-screen setup] in advance. (Multi display mode)

NOTE

- The IP image displayed in the multi-screen is only JPEG.

- The image in multi-screen will be stretched vertically to match the display frame with aspect ratio of 4:3.

- It is not possible to transfer from the [Live] screen to the multi-screen in the following cases.

  - When the power of this unit is turned off while displaying the IP image

  - When the network cable is disconnected

- The IP image display border is not displayed in red even if a tally signal (R tally) is input to the unit in the multi-screen.

Top of the page