- Top
- Description of Parts
- Front side

# Front side

1. Front tally lamp

   Lights up when the tally signal is supplied.

   Blinks in red while displaying warning, and blinks in green during the firmware update.

   NOTE

   - The brightness can be set with [MAIN MENU] → [SWITCH MODE] → [TALLY] → [FRONT TALLY]. Blinks in green [LOW] regardless of setting during the firmware update.

2. Lens mount (2/3 type bayonet)

   This is where the lens is mounted.

3. Lens fixing lever

   Fix the lens by turning the lever clockwise after mounting the lens to the lens mount.

Top of the page