- Top
- Operation
- Image quality adjustment
- Color correction function

# Color correction function

This function sets color saturation and phase. It applies individual effect on 12 phases in an image.

It can be set to individual color hue.

#### General settings

Use the camera with the factory settings.

#### Advanced settings

[G PHASE]/[CY-G PHASE]/[CY PHASE]/[B-CY PHASE]/[B PHASE]/[MG-B PHASE]/[MG_PHASE]/[R-MG PHASE]/[R PHASE]/[YL-R PHASE]/[YL PHASE]/[G-YL PHASE]: Changes the phase. + makes it go clockwise, and − makes it go counterclockwise.

[G SAT]/[CY-G SAT]/[CY SAT]/[B-CY SAT]/[B SAT]/[MG-B SAT]/[MG_SAT]/[R-MG SAT]/[R SAT]/[YL-R SAT]/[YL SAT]/[G-YL SAT]: Changes the saturation.

Top of the page